"OR007"|3|"GPI"|"Gravel pit"|"An open excavation from which soil and underlying material have been removed and used, without crushing, as a source of sand or gravel.  Typically 0.5 to 5 acres."|"143890"
"OR007"|3|"GRA"|"Gravelly spot"|"A spot where the surface layer has more than 35 percent, by volume, rock fragments that are mostly less than 3 inches in diameter in an area with less than 15 percent fragments.  Typically 0.5 to 5 acres."|"143891"
"OR007"|3|"LVS"|"Levee"|"An embankment that confines or controls water, especially one built along the banks of a river to prevent overflow of lowlands."|"143892"
"OR007"|3|"MPI"|"Mine or quarry"|"An open excavation from which soil and underlying material are removed and bedrock is exposed.  Also denotes surface openings to underground mines.  Typically 0.5 to 5 acres."|"143893"
"OR007"|3|"SLI"|"Slide or slip"|"A prominent landform scar or ridge caused by fairly recent mass movement or descent of earthy material resulting from failure of earth or rock under shear stress along one or several surfaces.  Typically 0.5 to 5 acres."|"143894"
