"10B"|"Chitwood silt loam, 0 to 7 percent slopes"||4|4||61|61|"None"|"None"|"0-14%"|5|9.34|17.84|26.34|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"|"3"|85|"3"|85|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"60843"
"10C"|"Chitwood silt loam, 7 to 15 percent slopes"||11|11||61|61|"None"|"None"|"0-14%"|5|9.34|17.84|26.34|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"|"4"|85|"4"|85|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Severe"|"Partially hydric"|1|"60844"
"11A"|"Coquille-Clatsop complex, 0 to 1 percent slopes"||1|1.3||15|15|"Frequent"|"Frequent"|"75-100%"|5.75|10.75|19.85|28.18|"Very poorly drained"|"Very poorly drained"|"D"||100|"6"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60845"
"12A"|"Coquille-Clatsop complex, protected, 0 to 1 percent slopes"||1|1.3||30|30|"Rare"|"Rare"|"75-100%"|5.75|10.75|20.11|28.78|"Very poorly drained"|"Very poorly drained"|"D"||100|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60846"
"13A"|"Coquille variant silt loam, 0 to 1 percent slopes"||1|1||30|30|"Rare"|"Rare"|"75-100%"|5|10|18.2|21.2|"Poorly drained"|"Poorly drained"|"D"|"3"|80|"3"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60847"
"14A"|"Croquib silt loam, 0 to 3 percent slopes"||2|2||0|5|"None"|"None"|"75-100%"|9.89|19.76|34.03|34.23|"Poorly drained"|"Poorly drained"|"D"||87|"4"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|0.98|"Slight"|"All hydric"|1|"60848"
"15"|"Dune land"|||2||0|0|"None"|"None"|"15-49%"|1.08|2.15|4.3|6.45||"Poorly drained"|"A"||85|"8"|85|"Not rated"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|||"Not rated"|1|"Not rated"|"Partially hydric"|1|"60849"
"16D"|"Ecola silt loam, 3 to 30 percent slopes"||17|17|102|||"None"|"None"|"0-14%"|7|12|22|22.4|"Well drained"|"Well drained"|"C"||95|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"60850"
"16F"|"Ecola-Templeton silt loams, 60 to 90 percent slopes"||75|75|102|||"None"|"None"|"0-14%"|6.86|12.12|22.74|27.71|"Well drained"|"Well drained"|"C"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60851"
"17A"|"Eilertsen silt loam, 0 to 3 percent slopes"||2|2||||"None"|"None"|"0-14%"|5.5|10.5|19.96|28.96|"Well drained"|"Well drained"|"B"||93|"2"|85|"Not limited"|"Not limited"|"Not limited"||"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Not limited"|||"Not limited"|0|"Slight"|"Partially hydric"|1|"60852"
"18B"|"Elsie silt loam, 0 to 7 percent slope"||4|4||||"None"|"None"|"0-14%"|6.25|11.25|21.25|30.89|"Well drained"|"Well drained"|"B"||90|"3"|85|"Not limited"|"Not limited"|"Not limited"||"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"60853"
"18C"|"Elsie silt loam, 7 to 15 percent slopes"||11|11||||"None"|"None"|"0-14%"|6.25|11.25|21.25|30.89|"Well drained"|"Well drained"|"B"||90|"4"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0|"Severe"|"Partially hydric"|1|"60854"
"19C"|"Gearhart fine sandy loam, 3 to 15 percent slopes"||9|9||||"None"|"None"|"0-14%"|4.35|6.43|9.43|12.43|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||92|"4"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"60855"
"19D"|"Gearhart fine sandy loam, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0-14%"|4.35|6.43|9.43|12.43|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.92|"Severe"|"Not hydric"|1|"60856"
"1D"|"Alstony gravelly loam, 3 to 30 percent slopes"||17|17|140|||"None"|"None"|"0-14%"|6.61|9.36|14.86|18.78|"Well drained"|"Well drained"|"B"||85|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Moderate"|"Partially hydric"|1|"60857"
"1E"|"Alstony gravelly loam, 30 to 60 percent slopes"||45|45|140|||"None"|"None"|"0-14%"|6.61|9.36|14.86|18.78|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60858"
"1F"|"Alstony gravelly loam, 60 to 90 percent slopes"||75|75|140|||"None"|"None"|"0-14%"|6.61|9.36|14.86|18.78|"Well drained"|"Well drained"|"B"||75|"7"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60859"
"20B"|"Grindbrook silt loam, 0 to 7 percent slopes"||4|4||76|76|"None"|"None"|"0-14%"|4.81|9.26|17.68|25.18|"Moderately well drained"|"Moderately well drained"|"C"|"2"|85|"2"|85|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"60860"
"20C"|"Grindbrook silt loam, 7 to 20 percent slopes"||14|14||76|76|"None"|"None"|"0-14%"|4.81|9.26|17.68|25.18|"Moderately well drained"|"Moderately well drained"|"C"||88|"3"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Partially hydric"|1|"60861"
"21D"|"Grindbrook silt loam, bedrock substratum, 3 to 30 percent slopes"||17|17|129|76|76|"None"|"None"|"0-14%"|5.5|10.5|20.5|26.3|"Moderately well drained"|"Moderately well drained"|"C"||88|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Partially hydric"|1|"60862"
"22F"|"Harslow-Kilchis very gravelly loams, 60 to 90 percent slopes"||75|75|48|||"None"|"None"|"0-14%"|5.33|7.2|9.01|9.01|"Well drained"|"Well drained"|"C"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60863"
"23A"|"Hebo silty clay loam, 0 to 3 percent slopes"||2|2||15|15|"None"|"None"|"75-100%"|4.76|8.82|16.86|25.36|"Poorly drained"|"Poorly drained"|"D"|"4"|85|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60864"
"24C"|"Heceta-Waldport fine sands, 0 to 15 percent slopes"||2|4.5||30|30|"None"|"None"|"50-74%"|2.65|4.15|7.15|10.15|"Poorly drained"|"Poorly drained"|"D"|"4"|50|"4"|50|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"Partially hydric"|1|"60865"
"25D"|"Hemcross silt loam, 3 to 30 percent slopes"||17|17||||"None"|"None"|"0-14%"|7.65|14.3|25.3|32.66|"Well drained"|"Well drained"|"B"||80|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"60866"
"26E"|"Hemcross-Klistan complex, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|7.3|12.46|20.21|25.88|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60867"
"27"|"Humitropepts, 25 to 60 percent slopes"||43|43|91|||"None"|"None"|"0-14%"|6.85|12|18.55|18.55|"Well drained"|"Well drained"|"C"||95|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60868"
"28"|"Humitropepts-Tropaquepts complex, 0 to 20 percent slopes"||10|6.4||0|0|"None"|"None"|"15-49%"|5.9|11.19|20.6|25.77|"Poorly drained"|"Poorly drained"|"D"||85|"4"|45|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0.47|"Severe"|"Partially hydric"|0.7|"60869"
"29F"|"Kilchis-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|6.41|7.65|7.65|7.65|"Well drained"|"Well drained"|"D"||80|"7"|45|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60870"
"2D"|"Anunde silt loam, 3 to 30 percent slopes"||17|17||||"None"|"None"|"0-14%"|7.8|15.26|29.26|42.9|"Well drained"|"Well drained"|"B"||89|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"60871"
"30A"|"Kirkendall silt loam, 0 to 3 percent slopes"||2|2||130|130|"Occasional"|"Occasional"|"0-14%"|5|10|20|29.54|"Well drained"|"Well drained"|"C"||92|"2"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Slight"|"Partially hydric"|0.6|"60872"
"31E"|"Klistan-Harslow complex, 30 to 60 percent slopes"||45|45|91|||"None"|"None"|"0-14%"|6.45|10.2|13.65|15.75|"Well drained"|"Well drained"|"B"||75|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60873"
"31F"|"Klistan-Harslow complex, 60 to 90 percent slopes"||75|75|91|||"None"|"None"|"0-14%"|6.38|10.22|13.65|15.51|"Well drained"|"Well drained"|"B"||75|"7"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60874"
"32D"|"Klootchie silt loam, 3 to 30 percent slopes"||17|17|114|||"None"|"None"|"0-14%"|8.25|15.75|27.27|29.79|"Well drained"|"Well drained"|"B"||88|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"60875"
"33E"|"Klootchie-Necanicum complex, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|8.44|16.23|27.06|37.88|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60876"
"34D"|"Klootchie-Necanicum complex, 3 to 30 percent slopes, bouldery"||17|17|114|||"None"|"None"|"0-14%"|7.7|13.87|23.37|25.66|"Well drained"|"Well drained"|"B"||85|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"60877"
"34E"|"Klootchie-Necanicum complex, 30 to 60 percent slopes, bouldery"||45|45|114|||"None"|"None"|"0-14%"|7.7|13.87|23.37|25.66|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60878"
"35B"|"Knappa silt loam, 0 to 7 percent slopes"||4|4||||"None"|"None"|"0-14%"|5.5|10.5|20.5|30.5|"Well drained"|"Well drained"|"B"|"2"|85|"2"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"60879"
"35C"|"Knappa silt loam, 7 to 15 percent slopes"||11|11||||"None"|"None"|"0-14%"|5.5|10.5|20.5|30.5|"Well drained"|"Well drained"|"B"|"2"|85|"2"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Partially hydric"|1|"60880"
"36C"|"Knappa variant loam, 3 to 15 percent slopes"||9|9||||"None"|"None"|"0-14%"|6.75|11.75|17.75|21.59|"Well drained"|"Well drained"|"B"|"3"|80|"3"|80|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"60881"
"37F"|"Laderly-Caterl complex, 60 to 90 percent slopes"||75|75|96|||"None"|"None"|"0-14%"|5.58|10.41|15.79|16.2|"Well drained"|"Well drained"|"C"||75|"7"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60882"
"38F"|"Laderly-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|5.31|8.11|10.19|10.19|"Well drained"|"Well drained"|"C"||75|"7"|40|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60883"
"39A"|"Locoda silt loam, 0 to 3 percent slopes"||2|2||15|15|"Frequent"|"Frequent"|"75-100%"|5.25|10.25|20.25|30.25|"Very poorly drained"|"Very poorly drained"|"D"||100|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60884"
"3F"|"Ascar-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|4.21|7.46|12.78|12.78|"Well drained"|"Well drained"|"C"||90|"7"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60885"
"4"|"Beaches"||2|2||0|0|"Very frequent"|"Very frequent"|"0-14%"|||||||"D"||100|"8"|100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|||"Not rated"||"Very Severe"|"All hydric"||"60886"
"40A"|"Locoda silt loam, protected, 0 to 3 percent slopes"||2|2||15|15|"Rare"|"Rare"|"75-100%"|5.25|10.25|20.25|30.25|"Very poorly drained"|"Very poorly drained"|"D"||100|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60887"
"41D"|"Mayger silt loam, 3 to 30 percent slopes"||17|17||69|69|"None"|"None"|"0-14%"|5|10|18.96|26.96|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60888"
"42D"|"McMille silt loam, 3 to 30 percent slopes"||17|17|114|||"None"|"None"|"0-14%"|7.11|12.44|22.44|25.24|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Not hydric"|1|"60889"
"42E"|"McMille silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|6.25|11.25|21.25|28.9|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60890"
"43A"|"McNulty silt loam, 0 to 3 percent slopes"||2|2||||"Frequent"|"Frequent"|"0-14%"|4.98|9.73|19.23|27.29|"Well drained"|"Well drained"|"B"||89|"2"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.4|"Slight"|"Partially hydric"|1|"60891"
"44E"|"Millicoma gravelly loam, 30 to 60 percent slopes"||45|45|101|||"None"|"None"|"0-14%"|4.85|7.75|11.75|11.83|"Well drained"|"Well drained"|"C"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60892"
"45A"|"Mues silt loam, 0 to 3 percent slopes"||1|1.1||64|64|"None"|"None"|"0-14%"|9.9|18.82|31.4|31.59|"Moderately well drained"|"Moderately well drained"|"C"||87|"2"|85|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Slight"|"Partially hydric"|0.99|"60893"
"46D"|"Murtip loam, 3 to 30 percent slopes"||17|17|127|||"None"|"None"|"0-14%"|10.15|17.77|29.27|34.22|"Well drained"|"Well drained"|"B"||75|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Not hydric"|1|"60894"
"47E"|"Murtip-Caterl complex, 30 to 60 percent slopes"||45|45|127|||"None"|"None"|"0-14%"|8.3|14.46|23.53|27.54|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60895"
"48E"|"Murtip-Caterl complex, 30 to 60 percent slopes, bouldery"||45|45|111|||"None"|"None"|"0-14%"|7.12|12.86|22.29|27.35|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60896"
"49A"|"Natal silty clay loam, 0 to 3 percent slopes"||2|2||8|8|"None"|"None"|"75-100%"|5|9.64|17.64|25.64|"Poorly drained"|"Poorly drained"|"D"||92|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60897"
"50E"|"Necanicum-Ascar complex, 30 to 60 percent slopes"||45|45|99|||"None"|"None"|"0-14%"|4.87|8.68|13.81|16.81|"Well drained"|"Well drained"|"B"||75|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60898"
"50F"|"Necanicum-Ascar complex, 60 to 90 percent slopes"||75|75|94|||"None"|"None"|"0-14%"|5.32|8.32|13.24|14.24|"Well drained"|"Well drained"|"B"||75|"7"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60899"
"51A"|"Nehalem silt loam, 0 to 3 percent slopes"||1|1||||"Frequent"|"Frequent"|"0-14%"|5|10|20|29.16|"Well drained"|"Well drained"|"B"|"2"|80|"2"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.4|"Slight"|"Partially hydric"|1|"60900"
"52A"|"Nestucca silt loam, 0 to 3 percent slopes"||2|2||46|46|"Frequent"|"Frequent"|"0-14%"|5|10|20|30|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"|"3"|85|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.44|"Slight"|"Partially hydric"|1|"60901"
"53D"|"Newanna gravelly loam, 3 to 30 percent slopes"||17|17|66|||"None"|"None"|"0-14%"|4.5|7.4|9|9|"Well drained"|"Well drained"|"C"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Moderate"|"Not hydric"|1|"60902"
"54F"|"Newanna-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|4.5|7.4|9|9|"Well drained"|"Well drained"|"C"||80|"7"|45|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60903"
"55B"|"Northrup silt loam, 0 to 7 percent slopes"||4|4||69|69|"None"|"None"|"0-14%"|5|10|20|28.48|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"3"|80|"3"|80|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|0.95|"60904"
"55C"|"Northrup silt loam, 7 to 15 percent slopes"||11|11||69|69|"None"|"None"|"0-14%"|5|10|20|28.48|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"3"|80|"3"|80|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Severe"|"Not hydric"|0.95|"60905"
"56D"|"Rinearson silt loam, 3 to 30 percent slopes"||17|17|132|||"None"|"None"|"0-14%"|5.75|10.75|20.75|27.15|"Well drained"|"Well drained"|"B"||88|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"60906"
"56E"|"Rinearson silt loam, 30 to 60 percent slopes"||45|45|124|||"None"|"None"|"0-14%"|5.5|10.5|20.5|25.3|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60907"
"56F"|"Rinearson silt loam, 60 to 90 percent slopes"||75|75|124|||"None"|"None"|"0-14%"|5.5|10.5|20.5|25.3|"Well drained"|"Well drained"|"B"||75|"7"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60908"
"57E"|"Scaponia-Braun silt loams, 30 to 60 percent slopes"||45|45|91|||"None"|"None"|"0-14%"|5.53|9.38|16.02|17.26|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60909"
"58D"|"Skipanon gravelly silt loam, 3 to 30 percent slopes"||17|17||||"None"|"None"|"0-14%"|5.85|10.11|17.59|26.11|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Not hydric"|1|"60910"
"58E"|"Skipanon gravelly silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|5.85|10.11|17.59|26.11|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60911"
"59D"|"Svensen loam, 3 to 30 percent slopes"||17|17||||"None"|"None"|"0-14%"|6.49|10.74|19.24|26.36|"Well drained"|"Well drained"|"B"||80|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"60912"
"59E"|"Svensen loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|10.4|20.4|29.13|36.25|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60913"
"59F"|"Svensen loam, 60 to 90 percent slopes"||75|75||||"None"|"None"|"0-14%"|6.49|10.74|19.24|26.36|"Well drained"|"Well drained"|"B"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60914"
"5A"|"Bergsvik mucky peat, 0 to 1 percent slopes"||1|1||8|8|"None"|"None"|"75-100%"|9.25|18|34.34|37.34|"Very poorly drained"|"Very poorly drained"|"D"||100|"5"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60915"
"60D"|"Templeton silt loam, 3 to 30 percent slopes"||18|18|150|||"None"|"None"|"0-14%"|8.25|14.91|26.41|37.91|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"60916"
"61E"|"Templeton-Ecola silt loams, 30 to 60 percent slopes"||45|45|91|||"None"|"None"|"0-14%"|8.36|14.88|25.87|34.49|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60917"
"62D"|"Tolany silt loam, 3 to 30 percent slopes"||17|17||||"None"|"None"|"0-14%"|8.25|15|27.5|40|"Well drained"|"Well drained"|"B"||88|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"60918"
"63D"|"Tolke silt loam, 3 to 30 percent slopes"||17|17||||"None"|"None"|"0-14%"|7.95|14.2|26.7|39.2|"Well drained"|"Well drained"|"B"||85|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"60919"
"64D"|"Tolke-Alstony complex, 3 to 30 percent slopes"||17|17|140|||"None"|"None"|"0-14%"|7.64|12.5|21.71|30.17|"Well drained"|"Well drained"|"B"||89|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"60920"
"65A"|"Treharne silt loam, 0 to 3 percent slopes"||2|2||76|76|"None"|"None"|"0-14%"|5|10|20|29.77|"Moderately well drained"|"Moderately well drained"|"C"||95|"2"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Slight"|"Partially hydric"|0.86|"60921"
"66"|"Tropofluvents, 0 to 3 percent slopes"||2|2||183|183|"Frequent"|"Frequent"|"0-14%"|3.65|6.41|11.41|16.41|"Well drained"|"Well drained"|"B"||90|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.4|"Slight"|"Partially hydric"|1|"60922"
"67"|"Tropopsamments, 0 to 15 percent slopes"||8|8||||"Rare"|"Rare"|"0-14%"|1.5|3|6|9|"Excessively drained"|"Excessively drained"|"A"||100|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Very limited"|1|"Moderate"|"Partially hydric"|1|"60923"
"68"|"Udifluvents-Hapludalfs, complex 0 to 15 percent slopes"||2|4.8||183|183|"Frequent"|"Frequent"|"0-14%"|4.17|7.59|13.77|19.23|"Somewhat excessively drained"|"Well drained"|"C"||85|"3"|45|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.21|"Slight"|"Not hydric"|0.89|"60924"
"69"|"Udipsamments, 0 to 15 percent slopes"||8|8||||"Rare"|"Rare"|"0-14%"|1.25|2.5|5|7.5|"Well drained"|"Well drained"|"A"||95|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Very limited"|1|"Moderate"|"Not hydric"|1|"60925"
"6A"|"Brallier mucky peat, 0 to 1 percent slopes"||1|1||8|8|"Frequent"|"Frequent"|"75-100%"|8.75|17.5|35|52.5|"Very poorly drained"|"Very poorly drained"|"D"||100|"5"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60926"
"70C"|"Waldport fine sand, 3 to 15 percent slopes"||9|9||||"None"|"None"|"0-14%"|1.5|3|6|9|"Excessively drained"|"Excessively drained"|"A"||92|"6"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Very limited"|1|"Moderate"|"Partially hydric"|1|"60927"
"70D"|"Waldport fine sand, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0-14%"|1.5|3|6|9|"Excessively drained"|"Excessively drained"|"A"||93|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Partially hydric"|1|"60928"
"71B"|"Walluski silt loam, 0 to 7 percent slopes"||3|3||69|69|"None"|"None"|"0-14%"|8.25|14.05|24.05|34.05|"Moderately well drained"|"Moderately well drained"|"C"|"3"|80|"2"|80|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"60929"
"71C"|"Walluski silt loam, 7 to 15 percent slopes"||11|11||69|69|"None"|"None"|"0-14%"|8.25|14.05|24.05|34.05|"Moderately well drained"|"Moderately well drained"|"C"|"4"|85|"3"|85|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Severe"|"Partially hydric"|1|"60930"
"71D"|"Walluski silt loam, 15 to 20 percent slopes"||18|18||76|76|"None"|"None"|"0-14%"|5.5|10.5|20.5|29.34|"Moderately well drained"|"Moderately well drained"|"C"||85|"3"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Partially hydric"|1|"60931"
"72A"|"Warrenton loamy fine sand, 0 to 3 percent slopes"||2|2||30|30|"None"|"None"|"75-100%"|5.3|7.52|11.52|15.52|"Very poorly drained"|"Very poorly drained"|"D"|"4"|85|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60932"
"73A"|"Wauna-Locoda silt loams, protected, 0 to 3 percent slopes"||2|2||15|15|"Rare"|"Rare"|"15-49%"|5.24|10.24|20.24|30.24|"Poorly drained"|"Very poorly drained"|"C"||93|"2"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|||"Not limited"|0.41|"Slight"|"All hydric"|0.78|"60933"
"7D"|"Braun-Scaponia silt loams, 3 to 30 percent slopes"||17|17|91|||"None"|"None"|"0-14%"|5.29|9.18|15.51|16.43|"Well drained"|"Well drained"|"C"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Not hydric"|1|"60934"
"7F"|"Braun-Scaponia silt loams, 60 to 90 percent slopes"||75|75|91|||"None"|"None"|"0-14%"|5.43|9.32|15.65|16.57|"Well drained"|"Well drained"|"C"||80|"7"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60935"
"8A"|"Brenner silt loam, 0 to 3 percent slopes"||1|1||15|15|"Frequent"|"Frequent"|"75-100%"|5|10|20|28.56|"Poorly drained"|"Poorly drained"|"D"||92|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"60936"
"9D"|"Caterl-Laderly complex, 3 to 30 percent slopes"||17|17|76|||"None"|"None"|"0-14%"|5.65|9.29|13.55|15.12|"Well drained"|"Well drained"|"B"||82|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Moderate"|"Partially hydric"|1|"60937"
"9E"|"Caterl-Laderly complex, 30 to 60 percent slopes"||45|45|76|||"None"|"None"|"0-14%"|5.63|9.23|13.37|14.87|"Well drained"|"Well drained"|"B"||75|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"60938"
"W"|"Water"|||||||||"0-14%"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|||"Not rated"||"Not rated"|"Unknown"||"60939"
"164F"|"Killam-Fawceter-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|6.62|11.25|16.37|18.86|"Well drained"|"Well drained"|"C"||85|"7"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"1723638"
"162E"|"Mosscreek-Fawceter complex, 30 to 60 percent slopes"||45|45|145|||"None"|"None"|"0-14%"|8.95|16.49|28.09|37.04|"Well drained"|"Well drained"|"B"||95|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"1723639"
"81B"|"Quillamook complex, 0 to 7 percent slopes"||3|3||||"None"|"None"|"0-14%"|10|20|35.44|42.47|"Well drained"|"Well drained"|"B"|"3"|85|"2"|85|"Not limited"|"Not limited"|"Not limited"||"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|0.76|"1723640"
