"31E"|"Tolovana-Templeton medial silt loams, 30 to 60 percent slopes"||45|45|150|||"None"|"None"|"0-14%"|9.52|18.4|28.71|38.5|"Well drained"|"Well drained"|"B"||75|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67123"
"31D"|"Tolovana-Templeton medial silt loams, 5 to 30 percent slopes"||18|18|150|||"None"|"None"|"0-14%"|9.26|17.68|28.24|38.38|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67124"
"303F"|"Ascar-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|4.21|7.46|12.78|12.78|"Well drained"|"Well drained"|"C"||90|"7"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67254"
"309D"|"Caterl-Laderly complex, 3 to 30 percent slopes"||17|17|76|||"None"|"None"|"0-14%"|5.65|9.29|13.55|15.12|"Well drained"|"Well drained"|"B"||82|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Moderate"|"Partially hydric"|1|"67255"
"314A"|"Croquib medial silt loam, 0 to 3 percent slopes"||2|2||0|5|"None"|"None"|"75-100%"|9.89|19.76|34.03|34.23|"Poorly drained"|"Poorly drained"|"D"||87|"4"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|0.98|"Slight"|"All hydric"|1|"67256"
"328"|"Dystrudepts-Humaquepts complex, 0 to 20 percent slopes"||10|6.4||0|0|"None"|"None"|"15-49%"|5.9|11.19|20.6|25.77|"Poorly drained"|"Poorly drained"|"D"||85|"4"|45|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0.47|"Severe"|"Partially hydric"|0.7|"67257"
"329F"|"Kilchis-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|6.41|7.65|7.65|7.65|"Well drained"|"Well drained"|"D"||80|"7"|45|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67258"
"338F"|"Laderly-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|5.31|8.11|10.19|10.19|"Well drained"|"Well drained"|"C"||75|"7"|40|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67259"
"345A"|"Mues medial silt loam, 0 to 3 percent slopes"||1|1.1||64|64|"None"|"None"|"0-14%"|9.9|18.82|31.4|31.59|"Moderately well drained"|"Moderately well drained"|"C"||87|"2"|85|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Slight"|"Partially hydric"|0.99|"67260"
"350E"|"Necanicum-Ascar complex, 30 to 60 percent slopes"||45|45|99|||"None"|"None"|"0-14%"|4.87|8.68|13.81|16.81|"Well drained"|"Well drained"|"B"||75|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67261"
"358D"|"Skipanon gravelly medial silt loam, 3 to 30 percent slopes"||17|17||||"None"|"None"|"0-14%"|5.85|10.11|17.59|26.11|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Not hydric"|1|"67262"
"358E"|"Skipanon gravelly medial silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|5.85|10.11|17.59|26.11|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67263"
"32D"|"Munsoncreek-Flowerpot complex, 5 to 30 percent slopes"||18|17.7|147|36|76|"None"|"None"|"0-14%"|8.28|13.64|22|29.86|"Well drained"|"Somewhat poorly drained"|"B"||87|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.35|"Severe"|"Partially hydric"|1|"67266"
"26F"|"Lebam-Necanicum complex, 60 to 90 percent slopes"||75|75||||"None"|"None"|"0-14%"|8.64|14.48|22.23|28.68|"Well drained"|"Well drained"|"B"||80|"7"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67267"
"25E"|"Lebam-Necanicum complex, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|8.94|14.94|22.93|29.51|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67268"
"62F"|"Rock outcrop-Laderly complex, 40 to 100 percent slopes"||70|68.5|0|||"None"|"None"|"0-14%"|5.31|8.11|10.19|10.19||"Well drained"|"D"||85|"8"|60|"Not rated"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|||"Not rated"|1|"Very Severe"|"Not hydric"|1|"67271"
"32E"|"Munsoncreek-Templeton medial silt loams, 30 to 60 percent slopes"||45|45|147|||"None"|"None"|"0-14%"|8.02|13.77|22.59|31.05|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67272"
"145F"|"Rock outcrop-Harslow complex, 40 to 100 percent slopes"||70|68.5|0|||"None"|"None"|"0-14%"|4.58|6.89|9.97|9.97||"Well drained"|"D"||85|"8"|60|"Not rated"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|||"Not rated"|1|"Very Severe"|"Not hydric"|1|"67273"
"119B"|"Oxyaquic Fulvudands-Typic Fulvudands complex, 0 to 7 percent slopes"||1|2.2||66|66|"Occasional"|"Occasional"|"0-14%"|10.06|19.58|25.48|26.88|"Moderately well drained"|"Moderately well drained"|"C"||95|"4"|75|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Slight"|"Partially hydric"|1|"67274"
"118B"|"Oxyaquic Hapludands-Alic Hapludands complex, 0 to 7 percent slopes"||1|2||64|64|"Occasional"|"Occasional"|"0-14%"|10.15|19.81|24.52|24.52|"Moderately well drained"|"Moderately well drained"|"B"||95|"4"|75|"Very limited"|"Very limited"||"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"||||0|"Slight"|"Partially hydric"|1|"67275"
"159D"|"Sevencedars very cobbly medial loam, clayey, 5 to 30 percent slopes"||18|18||||"None"|"None"|"0-14%"|5.31|9.81|16.49|21.49|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Moderate"|"Not hydric"|1|"67276"
"158E"|"Sevencedars very cobbly medial loam, till substratum, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|6.51|9.99|15.99|21.99|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67277"
"158D"|"Sevencedars very cobbly medial loam, till substratum, 5 to 30 percent slopes"||18|18||||"None"|"None"|"0-14%"|6.51|9.99|15.99|21.99|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Moderate"|"Not hydric"|1|"67278"
"157F"|"Caterl very cobbly medial loam, till substratum, 60 to 90 percent slopes"||75|75||||"None"|"None"|"0-14%"|4.95|8.56|15.06|19.41|"Well drained"|"Well drained"|"B"||80|"7"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67279"
"166F"|"Rock outcrop-Killam complex, 40 to 100 percent slopes"||70|68.5|0|||"None"|"None"|"0-14%"|5.85|10.35|13.47|13.47||"Well drained"|"D"||85|"8"|60|"Not rated"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|||"Not rated"|1|"Very Severe"|"Not hydric"|1|"67280"
"164F"|"Killam-Fawceter-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|6.62|11.25|16.37|18.86|"Well drained"|"Well drained"|"C"||85|"7"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67281"
"163F"|"Fawceter-Killam-Mosscreek complex, 60 to 90 percent slopes"||75|75|79|||"None"|"None"|"0-14%"|7.67|13.6|21.63|27.03|"Well drained"|"Well drained"|"B"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67282"
"162E"|"Mosscreek-Fawceter complex, 30 to 60 percent slopes"||45|45|145|||"None"|"None"|"0-14%"|8.95|16.49|28.09|37.04|"Well drained"|"Well drained"|"B"||95|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67283"
"162D"|"Mosscreek-Fawceter complex, 5 to 30 percent slopes"||18|18|145|||"None"|"None"|"0-14%"|9.03|16.72|28.56|37.71|"Well drained"|"Well drained"|"B"||90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67284"
"5E"|"Ferrelo loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|5.09|9.34|17.42|22.02|"Well drained"|"Well drained"|"B"||90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67286"
"6D"|"Horseprairie-Ferrelo complex, 3 to 20 percent slopes"||12|12||||"None"|"None"|"0-14%"|7.37|11.9|20.29|25.1|"Well drained"|"Well drained"|"B"||100|"3"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0|"Severe"|"Partially hydric"|1|"67287"
"8A"|"Depoe loam, 0 to 3 percent slopes"||1|1||8|8|"None"|"None"|"75-100%"|6.7|10.3|10.3|10.3|"Poorly drained"|"Poorly drained"|"D"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"67288"
"9D"|"Waldport fine sand, 5 to 30 percent slopes"||29|29||||"None"|"None"|"0-14%"|1|2|4|6|"Excessively drained"|"Excessively drained"|"A"||88|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Partially hydric"|1|"67289"
"11B"|"Netarts fine sandy loam, 0 to 5 percent slopes"||3|3||||"None"|"None"|"0-14%"|3.45|4.95|7.95|10.95|"Well drained"|"Well drained"|"B"||100|"4"|85|"Not limited"|"Not limited"|"Not limited"||"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"67290"
"11C"|"Netarts fine sandy loam, 3 to 12 percent slopes"||8|8||||"None"|"None"|"0-14%"|3.45|4.95|7.95|10.95|"Well drained"|"Well drained"|"B"||98|"4"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"67291"
"11E"|"Netarts fine sandy loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|3.45|4.95|7.95|10.95|"Well drained"|"Well drained"|"B"||90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67292"
"12B"|"Yaquina loamy fine sand, 0 to 5 percent slopes"||2|2||0|30|"None"|"None"|"75-100%"|3.27|4.77|7.77|10.77|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"||100|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"67293"
"14A"|"Heceta fine sand, 0 to 3 percent slopes"||1|1||0|0|"None"|"None"|"75-100%"|2.77|4.52|8.02|11.52|"Poorly drained"|"Poorly drained"|"D"||90|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"67294"
"24C"|"Lebam medial silt loam, 3 to 15 percent slopes"||7|7||||"None"|"None"|"0-14%"|10.15|16.75|25.75|32.85|"Well drained"|"Well drained"|"B"||85|"4"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Not hydric"|1|"67295"
"158F"|"Sevencedars very cobbly medial loam, till substratum, 60 to 90 percent slopes"||75|75||||"None"|"None"|"0-14%"|6.51|9.99|15.99|21.99|"Well drained"|"Well drained"|"B"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67296"
"120C"|"Alic Hapludands complex, 3 to 15 percent slopes"||6|7.8||||"None"|"None"|"0-14%"|8.37|15.16|23.47|25.63|"Well drained"|"Well drained"|"B"||100|"4"|95|"Not limited"|"Not limited"|"Not limited"||"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"67297"
"359E"|"Svensen medial loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|10.4|20.4|29.13|36.25|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67300"
"371C"|"Walluski silt loam, 7 to 15 percent slopes"||11|11||69|69|"None"|"None"|"0-14%"|8.25|14.05|24.05|34.05|"Moderately well drained"|"Moderately well drained"|"C"|"4"|85|"3"|85|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Severe"|"Partially hydric"|1|"67301"
"9E"|"Waldport fine sand, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|1|2|4|6|"Excessively drained"|"Excessively drained"|"A"||87|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Partially hydric"|1|"67302"
"101B"|"Urban land-Udorthents complex, 0 to 7 percent slopes, flooded"||3|2.8||36|36|"Occasional"|"Occasional"|"0-14%"|1.6|3.1|6.1|9.1||"Somewhat poorly drained"|"D"||100|"8"|65|"Not rated"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|||"Not rated"|0.92||"Partially hydric"|1|"67304"
"104A"|"Coquille-Brenner-Nehalem association, 0 to 3 percent slopes, protected"||0|0.5||36|36|"Rare"|"Rare"|"75-100%"|5|10|20|29.29|"Very poorly drained"|"Very poorly drained"|"D"|"4"|50|"4"|50|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|0.84|"Slight"|"Partially hydric"|0.96|"67305"
"89A"|"Udifluvents-Riverwash-Water complex, 0 to 3 percent slopes"||1|0.7||31|31|"Frequent"|"Frequent"|"0-14%"|3.29|6.04|11.48|15.98||"Somewhat excessively drained"|"A"||100|"4"|40|"Not rated"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Not rated"|||"Not rated"|0.4|"Slight"|"Partially hydric"|1|"67306"
"90A"|"Yachats very fine sandy loam, 0 to 3 percent slopes"||1|1||||"Frequent"|"Frequent"|"0-14%"|4.02|8.19|14.69|21.19|"Well drained"|"Well drained"|"A"|"3"|85|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.4|"Slight"|"Partially hydric"|1|"67307"
"28D"|"Templeton-Necanicum complex, 5 to 30 percent slopes"||18|18|150|||"None"|"None"|"0-14%"|7.39|13.32|22.9|32.49|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67309"
"9C"|"Waldport fine sand, 3 to 15 percent slopes"||8|8||||"None"|"None"|"0-14%"|1|2|4|6|"Excessively drained"|"Excessively drained"|"A"||90|"6"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Very limited"|1|"Moderate"|"Partially hydric"|1|"603896"
"181F"|"Neskowin-Rock outcrop-Necanicum complex, 60 to 100 percent slopes"||80|78.8|0|||"None"|"None"|"0-14%"|8.07|13.28|17.51|19.32|"Well drained"|"Well drained"|"C"||85|"7"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"603900"
"180F"|"Salander-Necanicum-Neskowin complex, 60 to 90 percent slopes"||75|75|71|||"None"|"None"|"0-14%"|8.98|16.87|27.94|37.35|"Well drained"|"Well drained"|"B"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"603901"
"180E"|"Salander-Necanicum complex, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|8.8|17.09|29.62|40.98|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"603902"
"180D"|"Salander medial silt loam, 5 to 30 percent slopes"||18|18||||"None"|"None"|"0-14%"|10.25|20.25|35.93|49.93|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"603903"
"517A"|"Euchre medial silt loam, 0 to 3 percent slopes"||1|1||36|36|"None"|"None"|"0-14%"|8.75|15.4|25.2|25.2|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"3"|85|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.92|"Slight"|"Partially hydric"|1|"603906"
"532D"|"Klootchie-Neotsu medial silt loams, 3 to 30 percent slopes"||15|15|81|||"None"|"None"|"0-14%"|10.26|20.12|30.54|38.41|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Severe"|"Not hydric"|1|"603907"
"110F"|"Waldport fine sand, thin surface, 60 to 90 percent slopes"||75|75||||"None"|"None"|"0-14%"|2.23|3.23|5.23|7.23|"Excessively drained"|"Excessively drained"|"A"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"741651"
"45B"|"Hebo silty clay loam, 0 to 5 percent slopes"||3|3||0|0|"None"|"None"|"75-100%"|4.4|8.15|16.43|26.43|"Poorly drained"|"Poorly drained"|"D"||90|"4"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Moderate"|"All hydric"|1|"741676"
"57C"|"Condorbridge gravelly medial loam, 3 to 15 percent slopes"||8|8||||"None"|"None"|"0-14%"|7.5|13.6|23.74|33.24|"Well drained"|"Well drained"|"B"||80|"3"|80|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0|"Moderate"|"Not hydric"|1|"741677"
"56C"|"Wolfer medial silt loam, 3 to 15 percent slopes"||9|9||||"None"|"None"|"0-14%"|10|19.3|31.3|31.3|"Well drained"|"Well drained"|"B"|"4"|85|"3"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"741678"
"81C"|"Quillamook complex, 3 to 15 percent slopes"||9|9||||"None"|"None"|"0-14%"|10|20|35.44|42.47|"Well drained"|"Well drained"|"B"|"4"|85|"3"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0|"Severe"|"Partially hydric"|0.76|"741679"
"91A"|"Gauldy loam, 0 to 3 percent slopes"||1|1||||"Frequent"|"Frequent"|"0-14%"|3.75|7.5|9.9|9.9|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||90|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.4|"Slight"|"Partially hydric"|1|"741680"
"92A"|"Yachats-Gauldy complex, 0 to 3 percent slopes"||1|1||||"Frequent"|"Frequent"|"0-14%"|3.89|7.87|12.44|15.88|"Well drained"|"Well drained"|"A"|"3"|45|"3"|45|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.4||"Partially hydric"|1|"741681"
"121D"|"Fendall-Munsoncreek medial silt loams, 5 to 30 percent slopes"||18|17|86|||"None"|"None"|"0-14%"|7.67|13.15|19.76|22.58|"Well drained"|"Well drained"|"C"||85|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Partially hydric"|1|"741686"
"178B"|"Fluventic Humic Dystrudepts-Dystrudepts-Aquepts complex, 0 to 5 percent slopes"||3|2.6||0|0|"Frequent"|"Frequent"|"15-49%"|5.61|10.56|20.11|23.16|"Moderately well drained"|"Poorly drained"|"C"||93|"3"|45|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.42|"Slight"|"Partially hydric"|0.84|"741688"
"181E"|"Neskowin-Salander medial loams, 30 to 60 percent slopes"||45|45|71|||"None"|"None"|"0-14%"|9.83|16.86|24.14|28.26|"Well drained"|"Well drained"|"C"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"741689"
"183D"|"Winema-Fendall medial silt loams, 5 to 30 percent slopes"||18|18|86|||"None"|"None"|"0-14%"|9.12|17.53|25.49|29.5|"Well drained"|"Well drained"|"B"||85|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"741690"
"182D"|"Neotsu-Salander medial loams, 5 to 30 percent slopes"||18|18|81|||"None"|"None"|"0-14%"|10.35|20.35|29.44|34.11|"Well drained"|"Well drained"|"C"||90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"741691"
"125B"|"Siletz medial silt loam, 0 to 7 percent slopes"||3|3||||"None"|"None"|"0-14%"|10|19.6|29.6|30.4|"Well drained"|"Well drained"|"B"|"3"|80|"2"|80|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|0.3|"741692"
"37E"|"Templeton-Skipanon complex, 30 to 60 percent slopes"||45|45|150|||"None"|"None"|"0-14%"|7.4|13.22|23.3|33.75|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"747146"
"51C"|"Walluski-Chitwood medial silt loams, 3 to 15 percent slopes"||9|9||28|48|"None"|"None"|"0-14%"|7.95|13.52|23.03|32.83|"Moderately well drained"|"Somewhat poorly drained"|"C"|"4"|45|"3"|75|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0.4|"Severe"|"Partially hydric"|1|"801115"
"185F"|"Udorthents-Rock outcrop complex, 60 to 100 percent slopes"||80|78.1|0|||"None"|"None"|"0-14%"|3.84|6.59|7.47|7.47|"Well drained"|"Well drained"|"C"||80|"7"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"801121"
"327"|"Dystrudepts, steep, 25 to 60 percent slopes"||43|43|91|||"None"|"None"|"0-14%"|6.85|12|18.55|18.55|"Well drained"|"Well drained"|"C"||95|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"801123"
"519D"|"Fendall-Winema medial silt loams, 15 to 35 percent slopes"||25|25|86|||"None"|"None"|"0-14%"|8.44|15.62|22.66|24.99|"Well drained"|"Well drained"|"C"||80|"4"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"801127"
"18C"|"Chitwood medial silt loam, 7 to 15 percent slopes"||11|11||28|48|"None"|"None"|"0-14%"|7.5|12.72|21.5|31|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"||85|"3"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Partially hydric"|1|"996247"
"33D"|"Tolovana medial silt loam, 5 to 30 percent slopes"||18|18||||"None"|"None"|"0-14%"|10.15|20.15|29.86|38.8|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"996294"
"54B"|"Knappa medial silt loam, 0 to 7 percent slopes"||3|3||||"None"|"None"|"0-14%"|7.5|15|25.1|34.74|"Well drained"|"Well drained"|"B"|"3"|85|"2"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|0.73|"996295"
"56B"|"Wolfer medial silt loam, 0 to 5 percent slopes"||3|3||||"None"|"None"|"0-14%"|10|19.3|31.3|31.3|"Well drained"|"Well drained"|"B"|"3"|80|"3"|80|"Not limited"|"Not limited"|"Not limited"||"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Slight"|"Partially hydric"|1|"996296"
"57B"|"Condorbridge gravelly medial loam, 0 to 7 percent slopes"||3|3||||"None"|"None"|"0-14%"|7.5|13.6|23.74|33.24|"Well drained"|"Well drained"|"B"||90|"2"|85|"Not limited"|"Not limited"|"Not limited"||"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|||"Not limited"|0|"Slight"|"Partially hydric"|1|"996297"
"94B"|"Ginger-Quillamook-Urban land complex, 0 to 7 percent slopes"||2|2.6||43|51|"None"|"None"|"0-14%"|10|19.25|30.8|39.32|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"|"4"|35|"3"|35|"Very limited"|"Very limited"||"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.34||"Partially hydric"|0.62|"997489"
"95B"|"Urban land-Quillamook complex, 0 to 7 percent slopes"||3|3||||"None"|"None"|"0-14%"|10|20|35.65|48.15||"Well drained"|"D"||60|"8"|55|||"Not limited"||"Not rated"|"Somewhat limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||||0|"Not rated"|"Partially hydric"|0.18|"997491"
"126B"|"Siletz medial silt loam, warm, 0 to 7 percent slopes"||3|3||||"None"|"None"|"0-14%"|10|19.6|29.6|30.4|"Well drained"|"Well drained"|"B"|"3"|80|"2"|80|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|0.3|"997494"
"128B"|"Siletz-Wolfer medial silt loams, 0 to 7 percent slopes"||3|3||||"None"|"None"|"0-14%"|10|19.46|30.4|30.82|"Well drained"|"Well drained"|"B"|"3"|85|"2"|45|"Somewhat limited"|"Somewhat limited"|"Not limited"||"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|0.63|"997495"
"127C"|"Condorbridge gravelly medial loam, warm, 3 to 15 percent slopes"||8|8||||"None"|"None"|"0-14%"|7.5|13.6|23.74|33.24|"Well drained"|"Well drained"|"B"||80|"3"|80|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0|"Moderate"|"Not hydric"|1|"997496"
"170B"|"Logsden-Nehalem silt loams, 0 to 5 percent slopes"||3|2.6||||"Rare"|"Frequent"|"0-14%"|5|10|20|29.63|"Well drained"|"Well drained"|"B"|"3"|90|"2"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|||"Not limited"|0.18|"Moderate"|"Partially hydric"|0.62|"997498"
"173C"|"Tillamook-Ginger medial silt loams, 3 to 15 percent slopes"||9|9||43|51|"None"|"None"|"0-14%"|10|19.34|29.9|37.6|"Moderately well drained"|"Somewhat poorly drained"|"D"|"4"|85|"3"|85|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"||||0.29|"Severe"|"Partially hydric"|1|"997499"
"190D"|"Mulkey medial loam, 5 to 30 percent slopes"||12|12|66|||"None"|"None"|"0-14%"|10.75|18.94|23.74|23.74|"Well drained"|"Well drained"|"C"||85|"6"|85|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Not hydric"|0.8|"997500"
"51B"|"Walluski-Chitwood medial silt loams, 0 to 7 percent slopes"||3|3||28|48|"None"|"None"|"0-14%"|7.9|13.42|22.85|32.61|"Moderately well drained"|"Somewhat poorly drained"|"D"|"3"|45|"2"|45|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0.47|"Moderate"|"Partially hydric"|1|"1427920"
"96B"|"Ginger-Hebo complex, 0 to 5 percent slopes"||2|2.5||0|0|"None"|"None"|"15-49%"|7.39|13.72|21.88|29.27|"Somewhat poorly drained"|"Poorly drained"|"D"|"4"|40|"3"|40|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.8|"Slight"|"Partially hydric"|1|"1427922"
"192A"|"Yachats very fine sandy loam, 0 to 3 percent slopes, occasional flooding"||2|2||||"Occasional"|"Occasional"|"0-14%"|4.02|8.19|14.69|21.19|"Well drained"|"Well drained"|"A"|"3"|85|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Slight"|"Partially hydric"|0.6|"1427923"
"191B"|"Siletz-Euchre medial silt loams, 0 to 7 percent slopes"||3|3||36|36|"None"|"None"|"0-14%"|9.42|17.64|27.55|27.97|"Well drained"|"Somewhat poorly drained"|"B"|"3"|40|"2"|40|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0.43|"Moderate"|"Partially hydric"|0.62|"1427924"
"359D"|"Svensen medial loam, 3 to 30 percent slopes"||17|17||||"None"|"None"|"0-14%"|10.4|20.4|29.13|36.25|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Not hydric"|1|"1427925"
"93B"|"Gauldy complex, 0 to 5 percent slopes"||1|1.8||||"Occasional"|"Occasional"|"0-14%"|3.75|7.5|9.9|9.9|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||85|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Slight"|"Not hydric"|1|"1427926"
"175D"|"Astoria medial silt loam, 5 to 30 percent slopes"||18|18|130|||"None"|"None"|"0-14%"|9.4|14.65|24.65|30.65|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67125"
"176D"|"Preacher-Bohannon complex, 5 to 35 percent slopes"||20|20|97|||"None"|"None"|"0-14%"|8.18|13.6|21.02|24.2|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.5|"Severe"|"Not hydric"|1|"67126"
"176E"|"Preacher-Bohannon complex, 35 to 60 percent slopes"||45|45|97|||"None"|"None"|"0-14%"|8.14|13.54|20.91|23.6|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67127"
"177B"|"Dystrudepts-Aquepts complex, 0 to 7 percent slopes"||3|3||0|0|"None"|"Frequent"|"15-49%"|5.51|10.46|19.36|28.36|"Moderately well drained"|"Poorly drained"|"C"||98|"2"|65|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.34|"Moderate"|"Partially hydric"|1|"67129"
"501D"|"Apt-McDuff complex, 5 to 30 percent slopes"||12|12|94|||"None"|"None"|"0-14%"|5.75|10.08|17.54|23.04|"Well drained"|"Well drained"|"B"||85|"6"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Not hydric"|1|"67131"
"501E"|"Apt-McDuff complex, 30 to 50 percent slopes"||40|40|94|||"None"|"None"|"0-14%"|5.75|10.1|17.54|22.85|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67132"
"532E"|"Klootchie-Neotsu medial silt loams, 30 to 60 percent slopes"||45|45|81|||"None"|"None"|"0-14%"|10.24|20.09|31.02|39.77|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67133"
"543F"|"Neotsu-Necanicum complex, 60 to 90 percent slopes"||75|75|81|||"None"|"None"|"0-14%"|8.02|15.31|20.74|23.07|"Well drained"|"Well drained"|"C"||75|"7"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67134"
"552F"|"Reedsport-Tolovana complex, 60 to 85 percent slopes"||75|75|86|||"None"|"None"|"0-14%"|10.21|18.92|26.14|29.49|"Well drained"|"Well drained"|"C"||80|"7"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67136"
"555D"|"Templeton-Fendall medial silt loams, 5 to 35 percent slopes"||20|20|86|||"None"|"None"|"0-14%"|7.99|14.23|23.71|31.15|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.5|"Severe"|"Not hydric"|1|"67137"
"556D"|"Tolovana-Reedsport complex, 3 to 35 percent slopes"||19|19|86|||"None"|"None"|"0-14%"|10.19|19.29|27.25|32.28|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.32|"Severe"|"Not hydric"|1|"67138"
"556E"|"Tolovana-Reedsport complex, 35 to 60 percent slopes"||48|48|86|||"None"|"None"|"0-14%"|10.19|19.34|27.41|32.66|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67139"
"611B"|"Dystrudepts-Aquepts-Humaquepts complex, warm, 0 to 7 percent slopes"||3|3||0|0|"None"|"Frequent"|"15-49%"|5.39|10.3|19.13|28.2|"Moderately well drained"|"Poorly drained"|"C"||95|"2"|50|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.49|"Moderate"|"Partially hydric"|1|"67140"
"70D"|"Murtip-Caterl-Laderly complex, 5 to 30 percent slopes"||18|18|76|||"None"|"None"|"0-14%"|7.93|13.64|21.72|25.13|"Well drained"|"Well drained"|"B"||90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67141"
"9B"|"Waldport fine sand, 0 to 5 percent slopes"||3|3||||"None"|"None"|"0-14%"|1|2|4|6|"Excessively drained"|"Excessively drained"|"A"||95|"6"|85||||"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"||||"Very limited"|1||"Partially hydric"|1|"67142"
"10B"|"Waldport fine sand, thin surface, 0 to 5 percent slopes"||3|3||||"None"|"None"|"0-14%"|2.23|3.23|5.23|7.23|"Excessively drained"|"Excessively drained"|"A"||95|"6"|85|"Not limited"|"Not limited"|"Not limited"||"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|||"Not limited"|0|"Slight"|"Partially hydric"|1|"67143"
"10C"|"Waldport fine sand, thin surface, 3 to 12 percent slopes"||9|9||||"None"|"None"|"0-14%"|2.23|3.23|5.23|7.23|"Excessively drained"|"Excessively drained"|"A"||95|"6"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"67144"
"10E"|"Waldport fine sand, thin surface, 15 to 60 percent slopes"||38|38||||"None"|"None"|"0-14%"|2.23|3.23|5.23|7.23|"Excessively drained"|"Excessively drained"|"A"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67145"
"17B"|"Chitwood-Hebo complex, 0 to 5 percent slopes"||2|2.4||0|0|"None"|"None"|"15-49%"|6.22|10.84|19.41|29.12|"Somewhat poorly drained"|"Poorly drained"|"D"||85|"3"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"Partially hydric"|1|"67146"
"50B"|"Walluski medial silt loam, 0 to 7 percent slopes"||3|3||69|69|"None"|"None"|"0-14%"|8.25|14.05|24.05|34.05|"Moderately well drained"|"Moderately well drained"|"C"|"3"|80|"2"|80|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"67147"
"7"|"Dune land"||38|38||||"None"|"None"|"0-14%"|1|2|4|6|||"A"||87|"8"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Very Severe"|"Partially hydric"||"67148"
"11D"|"Netarts fine sandy loam, 5 to 30 percent slopes"||18|18||||"None"|"None"|"0-14%"|3.45|4.95|7.95|10.95|"Well drained"|"Well drained"|"B"||90|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67149"
"13B"|"Waldport,thin surface-Heceta fine sands, 0 to 5 percent slopes"||3|2.7||0|0|"None"|"None"|"15-49%"|2.37|3.57|5.96|8.36|"Excessively drained"|"Poorly drained"|"A"||95|"6"|70|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|||"Not limited"|0.26|"Slight"|"Partially hydric"|1|"67150"
"15B"|"Netarts-Yaquina complex, 0 to 5 percent slopes"||3|2.5||0|30|"None"|"None"|"15-49%"|3.36|4.86|7.86|10.86|"Well drained"|"Somewhat poorly drained"|"B"||95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|||"Not limited"|0.47|"Moderate"|"Partially hydric"|1|"67151"
"29E"|"Templeton-Klootchie complex, 30 to 60 percent slopes"||45|45|150|||"None"|"None"|"0-14%"|9.14|17.26|29.94|42.62|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67153"
"29D"|"Templeton-Klootchie complex, 5 to 30 percent slopes"||18|18|150|||"None"|"None"|"0-14%"|9.03|16.97|29.5|42.03|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67154"
"37D"|"Templeton-Skipanon complex, 5 to 30 percent slopes"||18|18|150|||"None"|"None"|"0-14%"|7.29|12.99|22.88|33.19|"Well drained"|"Well drained"|"B"||75|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67156"
"38E"|"Templeton-Necanicum complex, 30 to 60 percent slopes"||45|45|150|||"None"|"None"|"0-14%"|7.04|12.68|21.5|30.33|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67157"
"55A"|"Histosols-Water complex, 0 to 1 percent slopes"||0.5|0.3||0|0|"Very frequent"|"Very frequent"|"50-74%"|11.25|22.5|32.75|42.75|"Very poorly drained"|"Very poorly drained"|"D"||100|"5"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1||"Partially hydric"|1|"67158"
"58C"|"Knappa medial silt loam, 3 to 15 percent slopes"||9|9||||"None"|"None"|"0-14%"|7.5|15|25.1|34.74|"Well drained"|"Well drained"|"B"|"4"|85|"3"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Severe"|"Partially hydric"|0.73|"67160"
"59B"|"Chitwood-Knappa medial silt loams, 0 to 7 percent slopes"||3|3||28|48|"None"|"None"|"0-14%"|7.5|13.79|23.19|32.76|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"||51|"3"|45|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|0.53|"Moderate"|"Partially hydric"|0.87|"67161"
"77A"|"Nestucca-Brenner silt loams, 0 to 3 percent slopes"||1|1||0|0|"Frequent"|"Frequent"|"15-49%"|5|10|20|29.06|"Somewhat poorly drained"|"Poorly drained"|"D"|"3"|55|"3"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.95|"Slight"|"Partially hydric"|1|"67162"
"99"|"Beaches"||2|2||0|0|"Very frequent"|"Very frequent"|"0-14%"|||||||"D"||95|"8"|95|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|||"Not rated"||"Very Severe"|"All hydric"||"67163"
"100B"|"Urban land-Udorthents complex, 0 to 7 percent slopes"||3|2.8||||"None"|"None"|"0-14%"|1.6|3.1|6.1|9.1||"Somewhat excessively drained"|"D"||100|"8"|65|||"Not limited"||"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|||||0||"Partially hydric"|0.9|"67164"
"116A"|"Aquepts, warm, 0 to 1 percent slopes"||0.5|0.5||0|0|"Frequent"|"Frequent"|"75-100%"|5.23|10.23|20.23|30.23|"Poorly drained"|"Poorly drained"|"D"||85|"5"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"67165"
"115A"|"Aquepts, 0 to 1 percent slopes"||0.5|0.5||0|0|"Frequent"|"Frequent"|"75-100%"|5.16|10.16|19.67|29.17|"Poorly drained"|"Poorly drained"|"D"||85|"5"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"67166"
"174C"|"Typic Fulvudands complex, 3 to 15 percent slopes"||6|7.8||||"None"|"None"|"0-14%"|8.93|16.78|28.09|32.9|"Well drained"|"Well drained"|"B"||100|"4"|95|"Not limited"|"Not limited"|"Not limited"||"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|1|"67168"
"342D"|"McMille medial silt loam, 3 to 30 percent slopes"||17|17|114|||"None"|"None"|"0-14%"|7.11|12.44|22.44|25.24|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Not hydric"|1|"67169"
"346D"|"Murtip medial loam, 3 to 30 percent slopes"||17|17|127|||"None"|"None"|"0-14%"|10.15|17.77|29.27|34.22|"Well drained"|"Well drained"|"B"||75|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Not hydric"|1|"67170"
"420F"|"Hembre medial silt loam, 60 to 90 percent slopes"||75|75|109|||"None"|"None"|"0-14%"|7.25|12.11|21.61|23.32|"Well drained"|"Well drained"|"B"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67171"
"420E"|"Hembre medial silt loam, 30 to 60 percent slopes"||45|45|109|||"None"|"None"|"0-14%"|7.25|12.11|21.61|23.32|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67172"
"425E"|"Klickitat stony loam, 30 to 60 percent slopes"||45|45|107|||"None"|"None"|"0-14%"|5.55|7.8|10.3|10.65|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67173"
"W"|"Water"||0|0||||||"0-14%"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|||"Not rated"||"Not rated"|"Unknown"||"67174"
"60E"|"Caterl-Laderly-Rock outcrop complex, 30 to 60 percent slopes"||45|45|0|||"None"|"None"|"0-14%"|5.63|9.24|13.4|14.91|"Well drained"|"Well drained"|"B"||90|"6"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67178"
"16F"|"Caterl-Laderly-Murtip complex, 60 to 90 percent slopes"||75|75|76|||"None"|"None"|"0-14%"|6.69|11.31|17.41|19.92|"Well drained"|"Well drained"|"B"||90|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67179"
"20E"|"Klootchie-Necanicum complex, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|8.44|16.23|27.06|37.88|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67180"
"44F"|"Harslow-Klistan-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|4.92|7.53|10.8|11.19|"Well drained"|"Well drained"|"C"||85|"7"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67181"
"157E"|"Caterl very cobbly medial loam, till substratum, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|4.95|8.56|15.06|19.41|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67182"
"44E"|"Klistan-Harslow-Rock outcrop complex, 30 to 60 percent slopes"||45|45|0|||"None"|"None"|"0-14%"|4.97|7.63|10.94|11.39|"Well drained"|"Well drained"|"B"||85|"6"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67183"
"61F"|"Laderly-Rock outcrop-Caterl complex, 60 to 90 percent south slopes"||75|75|0|||"None"|"None"|"0-14%"|5.51|8.81|12.18|13.11|"Well drained"|"Well drained"|"C"||85|"7"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67184"
"60F"|"Laderly-Caterl-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|5.59|9.08|12.95|14.24|"Well drained"|"Well drained"|"C"||85|"7"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67185"
"4E"|"Ginsberg-Klistan complex, 30 to 60 percent slopes"||45|45|112|||"None"|"None"|"0-14%"|8.04|13.88|21.17|26.25|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67186"
"4D"|"Ginsberg medial loam, 5 to 30 percent slopes"||18|18||||"None"|"None"|"0-14%"|8.95|15.75|24.3|30.8|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67187"
"403E"|"Astoria medial silt loam, 30 to 60 percent slopes"||45|45|130|||"None"|"None"|"0-14%"|9.4|14.65|24.65|30.65|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67189"
"433D"|"Melby silt loam, 5 to 30 percent slopes"||16|16|119|||"None"|"None"|"0-14%"|5.75|10.75|19.05|21.9|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.02|"Severe"|"Not hydric"|1|"67190"
"433E"|"Melby silt loam, 30 to 60 percent slopes"||45|45|119|||"None"|"None"|"0-14%"|5.75|10.75|19.05|21.9|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67191"
"439E"|"Tolke medial silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|7.95|14.2|26.7|39.2|"Well drained"|"Well drained"|"B"||70|"6"|70|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67192"
"307F"|"Braun-Scaponia silt loams, 60 to 90 percent slopes"||75|75|91|||"None"|"None"|"0-14%"|5.43|9.32|15.65|16.57|"Well drained"|"Well drained"|"C"||80|"7"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67193"
"322F"|"Harslow-Kilchis very gravelly medial loams, 60 to 90 percent slopes"||75|75|48|||"None"|"None"|"0-14%"|5.33|7.2|9.01|9.01|"Well drained"|"Well drained"|"C"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67194"
"347E"|"Murtip-Caterl complex, 30 to 60 percent slopes"||45|45|127|||"None"|"None"|"0-14%"|8.3|14.46|23.53|27.54|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67195"
"356D"|"Rinearson silt loam, 3 to 30 percent slopes"||17|17|132|||"None"|"None"|"0-14%"|5.75|10.75|20.75|27.15|"Well drained"|"Well drained"|"B"||88|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"67196"
"357E"|"Scaponia-Braun silt loams, 30 to 60 percent slopes"||45|45|91|||"None"|"None"|"0-14%"|5.53|9.38|16.02|17.26|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67197"
"363D"|"Tolke medial silt loam, 5 to 30 percent slopes"||17|17||||"None"|"None"|"0-14%"|7.95|14.2|26.7|39.2|"Well drained"|"Well drained"|"B"||85|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.08|"Severe"|"Partially hydric"|1|"67198"
"20D"|"Klootchie-Necanicum complex, 5 to 30 percent slopes"||18|18||||"None"|"None"|"0-14%"|8.73|16.85|28.2|39.55|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67199"
"19E"|"Klootchie medial silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0-14%"|10.15|19.91|33.91|47.91|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67200"
"43F"|"Klistan-Harslow-Hemcross complex, 60 to 90 percent slopes"||75|75|94|||"None"|"None"|"0-14%"|6.41|11.11|17.69|22.19|"Well drained"|"Well drained"|"B"||90|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67201"
"22F"|"Ascar-Necanicum-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|4.72|8.4|13.57|15.88|"Well drained"|"Well drained"|"C"||85|"7"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67202"
"21F"|"Necanicum-Ascar-Klootchie complex, 60 to 90 percent slopes"||75|75|99|||"None"|"None"|"0-14%"|6.13|11.34|18.56|24.2|"Well drained"|"Well drained"|"B"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67203"
"144F"|"Harslow-Rock outcrop-Klistan complex, 60 to 90 percent south slopes"||75|75|0|||"None"|"None"|"0-14%"|4.82|7.35|10.57|10.85|"Well drained"|"Well drained"|"C"||90|"7"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67205"
"23F"|"Rock outcrop-Ascar complex, 40 to 100 percent slopes"||70|68.5|0|||"None"|"None"|"0-14%"|4.21|7.46|12.78|12.78||"Well drained"|"D"||85|"8"|60|"Not rated"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|||"Not rated"|1|"Very Severe"|"Not hydric"|1|"67212"
"24D"|"Lebam medial silt loam, 5 to 30 percent slopes"||18|18||||"None"|"None"|"0-14%"|10.15|16.75|25.75|32.85|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67214"
"30D"|"Templeton medial silt loam, 5 to 30 percent slopes"||18|18|150|||"None"|"None"|"0-14%"|8.25|14.91|26.41|37.91|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67215"
"30E"|"Templeton-Ecola medial silt loams, 30 to 60 percent slopes"||45|45|91|||"None"|"None"|"0-14%"|8.36|14.88|25.87|34.49|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67216"
"30F"|"Templeton-Ecola medial silt loams, 60 to 90 percent slopes"||75|75|91|||"None"|"None"|"0-14%"|8.46|14.86|25.38|31.47|"Well drained"|"Well drained"|"B"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67217"
"48D"|"Hemcross-Klistan complex, 5 to 30 percent slopes"||18|18|112|||"None"|"None"|"0-14%"|8.73|16.66|28.34|39.18|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67218"
"48E"|"Hemcross-Klistan complex, 30 to 60 percent slopes"||45|45|112|||"None"|"None"|"0-14%"|8.16|15.26|25.58|34.75|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67221"
"70E"|"Murtip-Caterl-Laderly complex, 30 to 60 percent slopes"||45|45|76|||"None"|"None"|"0-14%"|7.8|13.4|21.28|24.59|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67225"
"71D"|"McMille-Mutt medial silt loams, 5 to 30 percent slopes"||18|18|64|||"None"|"None"|"0-14%"|7.05|12.35|19.38|21.03|"Well drained"|"Well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Severe"|"Not hydric"|1|"67229"
"72D"|"Caterl-Murtip complex, clayey, 5 to 30 percent slopes"||18|18|127|||"None"|"None"|"0-14%"|5.86|10.53|17.52|21.56|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Moderate"|"Not hydric"|1|"67230"
"156F"|"Sevencedars-Newanna complex, 60 to 90 percent slopes"||75|75|97|||"None"|"None"|"0-14%"|6.09|9.31|14.85|18.73|"Well drained"|"Well drained"|"B"||85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67231"
"157D"|"Caterl very cobbly medial loam, till substratum, 5 to 30 percent slopes"||18|18||||"None"|"None"|"0-14%"|4.95|8.56|15.06|19.41|"Well drained"|"Well drained"|"B"||80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Moderate"|"Not hydric"|1|"67232"
"161D"|"Sevencedars-Newanna-Woodspoint complex, 5 to 30 percent slopes"||18|18|97|||"None"|"None"|"0-14%"|7.12|12.07|19.17|23.03|"Well drained"|"Well drained"|"B"||90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.18|"Moderate"|"Not hydric"|1|"67234"
"161E"|"Sevencedars-Newanna-Woodspoint complex, 30 to 60 percent slopes"||45|45|97|||"None"|"None"|"0-14%"|7.05|11.74|18.67|23.23|"Well drained"|"Well drained"|"B"||90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67235"
"161F"|"Newanna-Sevencedars-Rock outcrop complex, 60 to 90 percent slopes"||75|75|0|||"None"|"None"|"0-14%"|5.91|9.02|14.37|17.37|"Well drained"|"Well drained"|"C"||90|"7"|70|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67236"
"309E"|"Caterl-Laderly complex, 30 to 60 percent slopes"||45|45|76|||"None"|"None"|"0-14%"|5.63|9.23|13.37|14.87|"Well drained"|"Well drained"|"B"||75|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Severe"|"Not hydric"|1|"67237"
"1A"|"Brenner silt loam, 0 to 1 percent slopes"||1|1||0|0|"Frequent"|"Frequent"|"75-100%"|5|10|20|29.04|"Poorly drained"|"Poorly drained"|"D"||85|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"67239"
"2A"|"Fluvaquents-Histosols complex, 0 to 1 percent slopes"||0.5|0.5||0|0|"Very frequent"|"Very frequent"|"75-100%"|7.3|14.61|23.51|28.7|"Very poorly drained"|"Very poorly drained"|"D"||98|"5"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1||"All hydric"|1|"67240"
"3A"|"Coquille silt loam, 0 to 1 percent slopes"||0.5|0.5||0|15|"Very frequent"|"Very frequent"|"75-100%"|5|10|20|29.48|"Very poorly drained"|"Very poorly drained"|"D"||95|"5"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1||"All hydric"|1|"67241"
"18B"|"Chitwood medial silt loam, 0 to 7 percent slopes"||3|3||28|48|"None"|"None"|"0-14%"|7.5|12.72|21.5|31|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"||85|"3"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Moderate"|"Partially hydric"|1|"67242"
"73A"|"Nehalem silt loam, 0 to 3 percent slopes, frequently flooded"||1|1||||"Frequent"|"Frequent"|"0-14%"|5|10|20|29.16|"Well drained"|"Well drained"|"B"|"3"|75|"3"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.4|"Slight"|"Partially hydric"|1|"67243"
"74A"|"Nehalem silt loam, 0 to 3 percent slopes"||1|1||||"Frequent"|"Frequent"|"0-14%"|5|10|20|29.16|"Well drained"|"Well drained"|"B"|"2"|80|"2"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.4|"Slight"|"Partially hydric"|1|"67244"
"76A"|"Nestucca silt loam, 0 to 3 percent slopes"||1|1||36|36|"Frequent"|"Frequent"|"0-14%"|5|10|20|29.08|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"|"3"|90|"3"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Somewhat limited"|0.92|"Slight"|"Partially hydric"|1|"67246"
"80B"|"Quillamook medial silt loam, 0 to 7 percent slopes"||3|3||||"None"|"None"|"0-14%"|10|20|35.65|48.15|"Well drained"|"Well drained"|"B"|"3"|80|"2"|80|"Not limited"|"Not limited"|"Not limited"||"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|0.18|"67247"
"81B"|"Quillamook complex, 0 to 7 percent slopes"||3|3||||"None"|"None"|"0-14%"|10|20|35.44|42.47|"Well drained"|"Well drained"|"B"|"3"|85|"2"|85|"Not limited"|"Not limited"|"Not limited"||"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|||"Not limited"|0|"Moderate"|"Partially hydric"|0.76|"67248"
"102A"|"Fluvaquents-Histosols complex, 0 to 1 percent slopes, diked"||0.5|0.5||0|0|"Frequent"|"Frequent"|"75-100%"|7.3|14.61|23.51|28.7|"Very poorly drained"|"Very poorly drained"|"D"||100|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"67249"
"103A"|"Coquille silt loam, 0 to 1 percent slopes, diked"||0|0||0|15|"Frequent"|"Frequent"|"75-100%"|5|10|20|29.48|"Very poorly drained"|"Very poorly drained"|"D"|"4"|85|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Very limited"|1|"Slight"|"All hydric"|1|"67250"
"170A"|"Logsden silt loam, 0 to 3 percent slopes"||1|1||||"Rare"|"Rare"|"0-14%"|5|10|20|30|"Well drained"|"Well drained"|"B"|"2"|85|"2"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Very limited"|||"Not limited"|0|"Slight"|"Partially hydric"|0.32|"67251"
"173B"|"Tillamook-Ginger medial silt loams, 0 to 7 percent slopes"||3|2.5||43|51|"None"|"None"|"0-14%"|10|19.34|29.9|37.6|"Moderately well drained"|"Somewhat poorly drained"|"D"|"3"|45|"2"|45|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|||"Not limited"|0.29|"Moderate"|"Partially hydric"|1|"67253"
