08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Chitwood component makes up 40 percent of the map unit. Slopes are 0 to 7 percent. This component is on fluviomarine terraces, stream terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 11 inches during January, February, December. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"1427920:1325228"|"1427920:1687143"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Walluski component makes up 45 percent of the map unit. Slopes are 0 to 7 percent. This component is on fluviomarine terraces, stream terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 27 inches during January, February, March, April, November, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"1427920:1325229"|"1427920:1687142"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"1427920:1342703"|"1427920:1687144"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Hebo component makes up 35 percent of the map unit. Slopes are 0 to 5 percent. This component is on depressions, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, December. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 4e.  This soil meets hydric criteria."|"1427922:1325235"|"1427922:1687225"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ginger component makes up 40 percent of the map unit. Slopes are 0 to 5 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 17 inches during January, February, December. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"1427922:1543477"|"1427922:1687224"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Yachats, occasional flooding component makes up 85 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria."|"1427923:1325241"|"1427923:1687357"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"1427923:1350001"|"1427923:1687358"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Euchre component makes up 35 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 36 to 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 14 inches during January, February, March, April, December. Organic matter content in the surface horizon is about 12 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"1427924:1325239"|"1427924:1687355"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Siletz component makes up 40 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"1427924:1325240"|"1427924:1687354"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Croquib soil is a minor component."|"1427924:1349978"|"1427924:1687356"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Svensen component makes up 85 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"1427925:1325244"|"1427925:1687395"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Gauldy, occasional flooding component makes up 50 percent of the map unit. Slopes are 0 to 5 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 30 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"1427926:1325255"|"1427926:1687214"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Gauldy, rare flooding component makes up 35 percent of the map unit. Slopes are 0 to 5 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 30 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria."|"1427926:1325256"|"1427926:1687215"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldport component makes up 85 percent of the map unit. Slopes are 3 to 15 percent. This component is on dunes on coastal plains, dunes on marine terraces. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"603896:1178736"|"603896:836147"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Heceta soil is a minor component."|"603896:1341131"|"603896:1687044"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"603900:1113350"|"603900:1687345"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Neskowin component makes up 35 percent of the map unit. Slopes are 60 to 100 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"603900:1113351"|"603900:1687344"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 20 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"603900:1113361"|"603900:1687346"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 20 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"603901:1113346"|"603901:1687340"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Salander component makes up 50 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and resdiuum derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"603901:1113347"|"603901:1687339"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Neskowin component makes up 15 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"603901:1113348"|"603901:1687341"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 25 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"603902:1113341"|"603902:1687338"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Salander component makes up 60 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and resdiuum derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"603902:1113342"|"603902:1687337"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Salander component makes up 85 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and resdiuum derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"603903:1113340"|"603903:1687336"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Euchre component makes up 85 percent of the map unit. Slopes are 0 to 3 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 36 to 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 14 inches during January, February, March, April, December. Organic matter content in the surface horizon is about 12 percent.  Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria."|"603906:1161456"|"603906:1687412"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"603906:1585297"|"603906:1687413"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Neotsu component makes up 35 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"603907:1161460"|"603907:1687417"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootchie component makes up 45 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"603907:1161461"|"603907:1687416"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 25 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67123:1113219"|"67123:1687110"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolovana component makes up 50 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes, hillslopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67123:1113220"|"67123:1687109"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolovana component makes up 45 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67124:1113218"|"67124:1687107"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 40 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67124:1166124"|"67124:1687108"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Astoria component makes up 80 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67125:1113326"|"67125:1687324"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Bohannon component makes up 20 percent of the map unit. Slopes are 5 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67126:1113327"|"67126:1687326"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Preacher component makes up 65 percent of the map unit. Slopes are 5 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67126:1113328"|"67126:1687325"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Bohannon component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67127:1113329"|"67127:1687328"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Preacher component makes up 55 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67127:1113330"|"67127:1687327"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Aquepts component makes up 30 percent of the map unit. Slopes are 0 to 7 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 5e.  This soil meets hydric criteria."|"67129:1113337"|"67129:1687330"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Dystrudepts component makes up 65 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 22 inches during January, February, March, April, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 2e.  This soil does not meet hydric criteria."|"67129:1113338"|"67129:1687329"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"67129:1137722"|"67129:1687331"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Apt component makes up 55 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67131:128498"|"67131:743140"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The McDuff component makes up 30 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67131:128499"|"67131:743146"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Apt component makes up 50 percent of the map unit. Slopes are 30 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67132:1080450"|"67132:1701241"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The McDuff component makes up 30 percent of the map unit. Slopes are 30 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67132:1080451"|"67132:1701242"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Neotsu component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67133:1161462"|"67133:1687419"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootchie component makes up 50 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67133:1161463"|"67133:1687418"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 35 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67134:1161466"|"67134:1687421"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Neotsu component makes up 40 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67134:1161467"|"67134:1687420"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolovana component makes up 30 percent of the map unit. Slopes are 60 to 85 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67136:1161471"|"67136:1687423"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Reedsport component makes up 50 percent of the map unit. Slopes are 60 to 85 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67136:1161472"|"67136:1687422"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fendall component makes up 30 percent of the map unit. Slopes are 5 to 35 percent. This component is on mountains, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 12 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67137:1161475"|"67137:1687425"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 55 percent of the map unit. Slopes are 5 to 35 percent. This component is on mountains, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67137:1161476"|"67137:1687424"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Reedsport component makes up 35 percent of the map unit. Slopes are 3 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67138:1161478"|"67138:1687427"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolovana component makes up 45 percent of the map unit. Slopes are 3 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67138:1161479"|"67138:1687426"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Reedsport component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67139:1161480"|"67139:1687429"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolovana component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67139:1161481"|"67139:1687428"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Humaquepts, warm component makes up 15 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, November, December. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 4e.  This soil meets hydric criteria."|"67140:1146373"|"67140:804741"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Aquepts, warm component makes up 30 percent of the map unit. Slopes are 0 to 7 percent. This component is on flood plains, valleys. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 5e.  This soil meets hydric criteria."|"67140:1146374"|"67140:804740"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Dystrudepts, warm component makes up 50 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, valleys. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 22 inches during January, February, March, April, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 2e.  This soil does not meet hydric criteria."|"67140:1146375"|"67140:804733"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Murtip component makes up 45 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67141:129244"|"67141:88594"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl component makes up 30 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67141:129245"|"67141:88596"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Laderly component makes up 15 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67141:129246"|"67141:88601"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Heceta soil is a minor component."|"67142:1151149"|"67142:1687042"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldport component makes up 85 percent of the map unit. Slopes are 0 to 5 percent. This component is on dunes on coastal plains, dunes on marine terraces. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67142:1178733"|"67142:836144"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldport, thin surface component makes up 85 percent of the map unit. Slopes are 0 to 5 percent. This component is on dunes on coastal plains, dunes on marine terraces. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67143:1113162"|"67143:961490"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Heceta soil is a minor component."|"67143:1151185"|"67143:1687050"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldport, thin surface component makes up 90 percent of the map unit. Slopes are 3 to 12 percent. This component is on dunes on coastal plains, dunes on marine terraces. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67144:1113163"|"67144:961496"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Heceta soil is a minor component."|"67144:1151212"|"67144:1687052"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldport, thin surface component makes up 85 percent of the map unit. Slopes are 15 to 60 percent. This component is on dunes on coastal plains, dunes on marine terraces. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67145:1105407"|"67145:1687053"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Hebo component makes up 35 percent of the map unit. Slopes are 0 to 5 percent. This component is on depressions on stream terraces, drainageways on fluviomarine terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, December. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 4e.  This soil meets hydric criteria."|"67146:1113176"|"67146:1687072"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Chitwood component makes up 50 percent of the map unit. Slopes are 0 to 5 percent. This component is on fluviomarine terraces, stream terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 11 inches during January, February, December. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"67146:1113177"|"67146:961886"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Walluski component makes up 80 percent of the map unit. Slopes are 0 to 7 percent. This component is on fluviomarine terraces, stream terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 27 inches during January, February, March, April, November, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"67147:1113248"|"67147:1687140"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"67147:1151688"|"67147:1687141"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dune land is a miscellaneous area."|"67148:1113156"|"67148:961437"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Heceta soil is a minor component."|"67148:1151137"|"67148:1687039"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Netarts component makes up 90 percent of the map unit. Slopes are 5 to 30 percent. This component is on dunes on marine terraces, coastal plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67149:1113167"|"67149:1687057"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldport, thin surface component makes up 70 percent of the map unit. Slopes are 0 to 5 percent. This component is on dunes on coastal plains, dunes on marine terraces. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67150:1113170"|"67150:961661"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Heceta component makes up 25 percent of the map unit. Slopes are 0 to 3 percent. This component is on depressions, coastal plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, November, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil meets hydric criteria."|"67150:1113172"|"67150:1687063"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Yaquina component makes up 45 percent of the map unit. Slopes are 0 to 5 percent. This component is on coastal plains, depressions. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil meets hydric criteria."|"67151:1113174"|"67151:961854"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Netarts component makes up 50 percent of the map unit. Slopes are 0 to 5 percent. This component is on dunes on marine terraces, coastal plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67151:1113175"|"67151:961857"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootchie component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67153:1113215"|"67153:1687101"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 45 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67153:1113216"|"67153:1687100"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootchie component makes up 35 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67154:1113213"|"67154:1687099"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 50 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67154:1113214"|"67154:1687098"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Skipanon component makes up 30 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of mass movement deposits derived from a mixture of igneous and sedimentary rock types overlying sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67156:1105410"|"67156:946657"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 45 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67156:1105411"|"67156:946655"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 35 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67157:1113233"|"67157:1687122"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 50 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67157:1113234"|"67157:1687121"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"67158:1113252"|"67158:1687151"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Histosols component makes up 55 percent of the map unit. Slopes are 0 to 1 percent. This component is on swamps, lowlands. The parent material consists of organic material and/or organic materials overlying alluvium and/or stratified organic materials and alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is very frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 90 percent.  Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.  The soil has a very slightly saline horizon within 30 inches of the soil surface."|"67158:1113253"|"67158:1687150"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Knappa component makes up 85 percent of the map unit. Slopes are 3 to 15 percent. This component is on stream terraces, fluviomarine terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"67160:1105412"|"67160:963622"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"67160:1151724"|"67160:1687160"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Knappa component makes up 40 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, fluviomarine terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"67161:1113255"|"67161:1687162"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Chitwood component makes up 45 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, fluviomarine terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 11 inches during January, February, December. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"67161:1113256"|"67161:1687161"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"67161:1151725"|"67161:1687163"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Brenner component makes up 40 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 4w.  This soil meets hydric criteria."|"67162:1544222"|"67162:1687194"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Nestucca component makes up 55 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 14 inches during January, February, March, April, May, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria."|"67162:1544225"|"67162:1687193"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaches is a miscellaneous area."|"67163:1121472"|"67163:1687226"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Udorthents component makes up 25 percent of the map unit. Slopes are 0 to 7 percent. This component is on flood plains, stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock and/or colluvium derived from igneous rock and human transported materials. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent.  Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria."|"67164:1113276"|"67164:1687228"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Urban land is a miscellaneous area."|"67164:1113277"|"67164:1687227"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Aquents soil is a minor component."|"67164:1345222"|"67164:1687229"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Aquepts, warm component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 5w.  This soil meets hydric criteria."|"67165:1113291"|"67165:1687245"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Aquepts component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 12 percent.  Nonirrigated land capability classification is 5w.  This soil meets hydric criteria."|"67166:1113290"|"67166:1687244"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Fulvudands, fan component makes up 35 percent of the map unit. Slopes are 3 to 15 percent. This component is on fans, river valleys. The parent material consists of debris flow deposits derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67168:1121454"|"67168:1687322"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Fulvudands, terrace component makes up 60 percent of the map unit. Slopes are 3 to 15 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 30 to 50 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67168:1147689"|"67168:1687321"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Croquib soil is a minor component."|"67168:1147694"|"67168:1687323"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The McMille component makes up 85 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67169:1161337"|"67169:1687380"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Murtip component makes up 75 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and resdiuum derived from igneous rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67170:1161339"|"67170:1687384"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Hembre component makes up 85 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67171:1161430"|"67171:1687403"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Hembre component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67172:1161429"|"67172:1687402"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klickitat component makes up 80 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria."|"67173:1161431"|"67173:1687404"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"67174:1121769"|"67174:1687021"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67178:1113257"|"67178:1687166"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Laderly component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67178:1113258"|"67178:1687165"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl component makes up 35 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67178:1113259"|"67178:1687164"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Laderly component makes up 25 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67179:94114"|"67179:71597"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl component makes up 45 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67179:94115"|"67179:71600"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Murtip component makes up 20 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67179:94118"|"67179:71603"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67180:93972"|"67180:89260"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootchie component makes up 55 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67180:93974"|"67180:89270"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klistan component makes up 30 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67181:94109"|"67181:1687130"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Harslow component makes up 35 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67181:94110"|"67181:88477"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67181:94112"|"67181:88518"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl, till substratum component makes up 80 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium overlying glacial till derived from igenous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67182:94046"|"67182:1687278"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67183:1113243"|"67183:1687128"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Harslow component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria."|"67183:1113244"|"67183:1687127"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klistan component makes up 35 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67183:1113245"|"67183:1687126"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl, south slopes component makes up 20 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67184:1113264"|"67184:1687172"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67184:1113265"|"67184:1687171"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Laderly, south slopes component makes up 40 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67184:1113266"|"67184:1687170"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl component makes up 30 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67185:93976"|"67185:89206"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Laderly component makes up 35 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67185:93977"|"67185:1687167"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67185:93979"|"67185:89220"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klistan component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67186:1113150"|"67186:961425"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ginsberg component makes up 60 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67186:1113151"|"67186:961423"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ginsberg component makes up 85 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67187:109081"|"67187:82153"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Astoria component makes up 80 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67189:93988"|"67189:1687401"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Melby component makes up 80 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67190:93995"|"67190:71497"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Melby component makes up 80 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67191:94001"|"67191:1687406"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolke component makes up 70 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock, and in some areas derived from igenous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67192:94007"|"67192:1687407"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Braun component makes up 45 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67193:129258"|"67193:1687361"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Scaponia component makes up 35 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67193:129259"|"67193:1687362"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Harslow component makes up 50 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67194:94012"|"67194:1687370"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Kilchis component makes up 35 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 12 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67194:94013"|"67194:1687371"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Murtip component makes up 45 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and resdiuum derived from igneous rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67195:94020"|"67195:1687385"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl component makes up 35 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67195:94021"|"67195:1687386"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Rinearson component makes up 85 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and resdiuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67196:94027"|"67196:1687389"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Aquepts soil is a minor component."|"67196:94029"|"67196:1687390"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Scaponia component makes up 50 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67197:94033"|"67197:1687391"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Braun component makes up 35 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67197:94034"|"67197:1687392"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Aquands soil is a minor component."|"67198:1774728"|"67198:2220178"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolke component makes up 80 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock, and in some areas derived from igenous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67198:94041"|"67198:1687397"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootchie component makes up 60 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67199:93968"|"67199:89311"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 25 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67199:93969"|"67199:1687080"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootchie component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67200:94119"|"67200:88266"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klistan component makes up 35 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67201:94124"|"67201:71611"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Harslow component makes up 30 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67201:94125"|"67201:1687124"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Hemcross component makes up 25 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67201:94128"|"67201:1687125"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 30 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67202:94129"|"67202:1687087"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ascar component makes up 35 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67202:94130"|"67202:1687086"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67202:94131"|"67202:1687088"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 40 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67203:94134"|"67203:1687083"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ascar component makes up 25 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67203:94135"|"67203:1687084"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootchie component makes up 20 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67203:94137"|"67203:1687085"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klistan, south slopes component makes up 20 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67205:94139"|"67205:1687272"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Harslow, south slopes component makes up 40 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67205:94140"|"67205:1687270"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67205:94141"|"67205:1687271"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ascar component makes up 25 percent of the map unit. Slopes are 40 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67212:133630"|"67212:1687090"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67212:133632"|"67212:1687089"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Lebam component makes up 85 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67214:109748"|"67214:1687091"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 85 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67215:94199"|"67215:1687102"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 60 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67216:94206"|"67216:82173"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ecola component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes, hillslopes. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67216:94207"|"67216:82178"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 45 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67217:94214"|"67217:808049"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ecola component makes up 40 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes, hillslopes. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67217:94215"|"67217:808054"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Hemcross component makes up 60 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67218:94143"|"67218:88491"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klistan component makes up 25 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67218:94144"|"67218:88492"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Hemcross component makes up 50 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67221:94148"|"67221:88497"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Klistan component makes up 35 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67221:94149"|"67221:88502"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Murtip component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67225:109738"|"67225:88575"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67225:109739"|"67225:88580"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Laderly component makes up 15 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67225:109740"|"67225:88585"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The McMille component makes up 50 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67229:94191"|"67229:88633"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Mutt component makes up 35 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67229:94192"|"67229:88638"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Murtip, clayey component makes up 20 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock overlying residuum weathered from tuff. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67230:94194"|"67230:71657"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl, clayey component makes up 60 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock overlying residuum weathered from tuff. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67230:94195"|"67230:71663"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Newanna component makes up 30 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67231:94168"|"67231:1687276"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Sevencedars component makes up 55 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67231:94169"|"67231:88699"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl, till substratum component makes up 80 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium overlying glacial till derived from igenous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67232:94155"|"67232:1687277"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Sevencedars component makes up 35 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67234:94178"|"67234:88655"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Newanna component makes up 30 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67234:94179"|"67234:88664"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodspoint component makes up 25 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67234:94180"|"67234:88665"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Sevencedars component makes up 50 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67235:94173"|"67235:84206"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Newanna component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67235:94174"|"67235:84211"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodspoint component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67235:94175"|"67235:84214"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Sevencedars component makes up 35 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67236:94157"|"67236:1687295"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Newanna component makes up 35 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67236:94158"|"67236:1687294"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67236:94159"|"67236:1687296"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67237:94216"|"67237:1687366"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Laderly component makes up 35 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67237:94217"|"67237:1687367"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Brenner component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 4w.  This soil meets hydric criteria."|"67239:1105406"|"67239:791213"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Humaquepts soil is a minor component."|"67240:1123448"|"67240:1687027"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tidal flats soil is a minor component."|"67240:877316"|"67240:1687026"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Histosols component makes up 35 percent of the map unit. Slopes are 0 to 1 percent. This component is on tidal marshes, lowlands. The parent material consists of organic material over estuarine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is very frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 90 percent.  Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.  The soil has a very slightly saline horizon within 30 inches of the soil surface."|"67240:877317"|"67240:1687024"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fluvaquents component makes up 60 percent of the map unit. Slopes are 0 to 1 percent. This component is on tidal marshes, lowlands. The parent material consists of estuarine deposits. Depth to a root restrictive layer, strongly contrasting textural stratification, is 30 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is very frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.  The soil has a very slightly saline horizon within 30 inches of the soil surface."|"67240:877318"|"67240:531252"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Histosols soil is a minor component."|"67241:1111821"|"67241:1687030"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"67241:877502"|"67241:1687029"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Coquille component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on tidal marshes, lowlands. The parent material consists of estuarine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is very frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, December. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 5w.  This soil meets hydric criteria."|"67241:877504"|"67241:531336"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Chitwood component makes up 80 percent of the map unit. Slopes are 0 to 7 percent. This component is on fluviomarine terraces, stream terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 11 inches during January, February, December. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"67242:1113178"|"67242:961903"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"67242:1151337"|"67242:1687074"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Nehalem, frequently flooded component makes up 75 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria."|"67243:1113267"|"67243:1687187"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"67243:1151765"|"67243:1687188"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Nehalem component makes up 80 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 2w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria."|"67244:1113268"|"67244:1687189"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"67244:1130092"|"67244:1687190"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Nestucca component makes up 90 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 14 inches during January, February, March, April, May, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria."|"67246:1113269"|"67246:1687191"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"67246:1130612"|"67246:1687192"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Quillamook component makes up 80 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 17 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"67247:1151980"|"67247:1687195"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"67247:1343493"|"67247:1687196"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Quillamook component makes up 25 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 17 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"67248:1113272"|"67248:1687198"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Quillamook, gravelly substratum component makes up 60 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium overlying sandy and gravelly alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 17 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"67248:1113273"|"67248:1687197"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"67248:1160518"|"67248:1687199"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fluvaquents, diked component makes up 60 percent of the map unit. Slopes are 0 to 1 percent. This component is on tidal marshes, lowlands. The parent material consists of estuarine deposits. Depth to a root restrictive layer, strongly contrasting textural stratification, is 30 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 4w.  This soil meets hydric criteria.  The soil has a very slightly saline horizon within 30 inches of the soil surface."|"67249:1123343"|"67249:1687233"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Histosols, diked component makes up 35 percent of the map unit. Slopes are 0 to 1 percent. This component is on tidal marshes, lowlands. The parent material consists of organic material and/or organic materials overlying alluvium and/or stratified organic materials and alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, November, December. Organic matter content in the surface horizon is about 90 percent.  Nonirrigated land capability classification is 4w.  This soil meets hydric criteria.  The soil has a very slightly saline horizon within 30 inches of the soil surface."|"67249:1123344"|"67249:787248"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Coquille soil is a minor component."|"67249:1123351"|"67249:1687236"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Coquille, diked component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on tidal marshes, lowlands. The parent material consists of estuarine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, December. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria."|"67250:1113284"|"67250:1687237"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"67250:1152281"|"67250:1687239"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Histosols soil is a minor component."|"67250:1152282"|"67250:1687238"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Logsden component makes up 85 percent of the map unit. Slopes are 0 to 3 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 2w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria."|"67251:1113310"|"67251:1687310"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"67251:1161109"|"67251:1687311"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ginger component makes up 40 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 17 inches during January, February, December. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"67253:1113321"|"67253:1687316"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Tillamook component makes up 45 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 25 inches during January, February, March, December. Organic matter content in the surface horizon is about 17 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"67253:1152520"|"67253:1687315"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"67253:1152521"|"67253:1687317"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ascar component makes up 50 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67254:129250"|"67254:1687359"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67254:129251"|"67254:1687360"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl component makes up 45 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67255:127397"|"67255:1687363"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Laderly component makes up 35 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67255:127398"|"67255:1687364"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Aquands soil is a minor component."|"67255:1774726"|"67255:2220175"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Croquib component makes up 85 percent of the map unit. Slopes are 0 to 3 percent. This component is on stream terraces, river valleys. The parent material consists of mixed alluvium overlying weakly to strongly consolidated alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 25 to 40 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, December. Organic matter content in the surface horizon is about 13 percent.  Nonirrigated land capability classification is 4w.  This soil meets hydric criteria."|"67256:1161285"|"67256:1687368"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Humaquepts soil is a minor component."|"67256:1585073"|"67256:1687369"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Dystrudepts component makes up 45 percent of the map unit. Slopes are 0 to 20 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 63 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"67257:1152609"|"67257:1687373"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Humaquepts component makes up 40 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, November, December. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 4e.  This soil meets hydric criteria."|"67257:1152610"|"67257:1687374"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Croquib soil is a minor component."|"67257:1585083"|"67257:1687375"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67258:1161323"|"67258:1687377"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Kilchis component makes up 45 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 12 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67258:1161324"|"67258:1687376"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67259:1161332"|"67259:1687379"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Laderly component makes up 40 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67259:1161333"|"67259:1687378"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Mues component makes up 85 percent of the map unit. Slopes are 0 to 3 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium over consolidated gravelly alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 25 to 40 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 25 inches during January, February, March, April, May, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 2w.  This soil does not meet hydric criteria."|"67260:1161338"|"67260:1687381"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Croquib soil is a minor component."|"67260:1585133"|"67260:1687382"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Humaquepts soil is a minor component."|"67260:1585136"|"67260:1687383"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 45 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67261:1161399"|"67261:1687387"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ascar component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria."|"67261:1161402"|"67261:1687388"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Skipanon component makes up 80 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of mass movement deposits derived from a mixture of igneous and sedimentary rock types overlying sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67262:1161418"|"67262:1687393"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Skipanon component makes up 80 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of mass movement deposits derived from a mixture of igneous and sedimentary rock types overlying sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67263:1161421"|"67263:1687394"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Munsoncreek component makes up 65 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67266:109084"|"67266:1687111"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Flowerpot component makes up 20 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 14 inches during January, February. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67266:109085"|"67266:1687112"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Aquepts soil is a minor component."|"67266:1152120"|"67266:1687113"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 25 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67267:1113183"|"67267:962672"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Lebam component makes up 55 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67267:1113184"|"67267:1687094"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67268:1113181"|"67268:1687093"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Lebam component makes up 60 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67268:1113182"|"67268:962662"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Laderly component makes up 25 percent of the map unit. Slopes are 40 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67271:133635"|"67271:1687174"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67271:133637"|"67271:1687173"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Munsoncreek component makes up 65 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67272:109086"|"67272:88455"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67272:109087"|"67272:88460"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Harslow component makes up 25 percent of the map unit. Slopes are 40 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria."|"67273:128967"|"67273:89187"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67273:128969"|"67273:1687273"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Fulvudands, terrace component makes up 30 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 30 to 50 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67274:1113292"|"67274:1687252"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Oxyaquic Fulvudands, flood plain component makes up 45 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 12 to 20 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 26 inches during January, February, March, April, May, June, October, November, December. Organic matter content in the surface horizon is about 10 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67274:1113293"|"67274:1687251"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Croquib soil is a minor component."|"67274:1144907"|"67274:1687255"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"67274:1144908"|"67274:1687254"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Riverwash soil is a minor component."|"67274:1333738"|"67274:1687253"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Croquib soil is a minor component."|"67275:1130177"|"67275:1687250"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Riverwash soil is a minor component."|"67275:128933"|"67275:1687248"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Alic Hapludands, terrace component makes up 30 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, valleys. The parent material consists of alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 37 to 61 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria."|"67275:128934"|"67275:791295"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Oxyaquic Hapludands, flood plain component makes up 45 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, valleys. The parent material consists of alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 25 to 61 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 25 inches during January, February, March, April, May, November, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67275:128935"|"67275:791316"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"67275:1333706"|"67275:1687249"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Sevencedars, clayey component makes up 85 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock overlying residuum weathered from tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67276:129027"|"67276:1687283"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Sevencedars, till substratum component makes up 80 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium overlying glacial till derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67277:129018"|"67277:1349482"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Sevencedars, till substratum component makes up 80 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium overlying glacial till derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67278:129015"|"67278:1349483"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Caterl, till substratum component makes up 80 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium overlying glacial till derived from igenous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67279:129009"|"67279:89019"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67280:133656"|"67280:89074"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Killam component makes up 25 percent of the map unit. Slopes are 40 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67280:133657"|"67280:89085"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fawceter component makes up 30 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67281:133651"|"67281:89052"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Killam component makes up 35 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67281:133652"|"67281:89057"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"67281:133654"|"67281:89067"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fawceter component makes up 40 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67282:109090"|"67282:82155"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Killam component makes up 25 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67282:109091"|"67282:1687303"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Mosscreek component makes up 20 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67282:109092"|"67282:82166"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fawceter component makes up 45 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67283:133647"|"67283:1687301"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Mosscreek component makes up 50 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67283:133649"|"67283:89048"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Mosscreek component makes up 50 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67284:133643"|"67284:1687297"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fawceter component makes up 40 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67284:133644"|"67284:1687299"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ferrelo component makes up 90 percent of the map unit. Slopes are 30 to 60 percent. This component is on marine terraces, coastal plains. The parent material consists of eolian and/or marine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67286:1113153"|"67286:960590"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ferrelo component makes up 25 percent of the map unit. Slopes are 3 to 20 percent. This component is on marine terraces, coastal plains. The parent material consists of eolian and/or marine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"67287:1113154"|"67287:961388"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Horseprairie component makes up 65 percent of the map unit. Slopes are 3 to 20 percent. This component is on marine terraces, coastal plains. The parent material consists of eolian and/or marine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"67287:1113155"|"67287:961386"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Depoe soil is a minor component."|"67287:1151132"|"67287:1687037"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Depoe component makes up 85 percent of the map unit. Slopes are 0 to 3 percent. This component is on depressions on marine terraces, coastal plains. The parent material consists of loamy eolian deposits overlying stratified sandy marine deposits. Depth to a root restrictive layer, ortstein, is 12 to 20 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 3 inches during January, February, March, April, May, October, November, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria."|"67288:1113157"|"67288:961446"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldport component makes up 85 percent of the map unit. Slopes are 5 to 30 percent. This component is on dunes on coastal plains, dunes on marine terraces. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67289:1113160"|"67289:798064"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Heceta soil is a minor component."|"67289:1137541"|"67289:1687046"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Netarts component makes up 85 percent of the map unit. Slopes are 0 to 5 percent. This component is on dunes on marine terraces, coastal plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67290:1113164"|"67290:961520"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Yaquina soil is a minor component."|"67290:1151265"|"67290:2479820"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Heceta soil is a minor component."|"67290:1151269"|"67290:1687055"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Netarts component makes up 90 percent of the map unit. Slopes are 3 to 12 percent. This component is on dunes on marine terraces, coastal plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67291:1113166"|"67291:1687056"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Yaquina soil is a minor component."|"67291:1151278"|"67291:2479821"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Netarts component makes up 90 percent of the map unit. Slopes are 30 to 60 percent. This component is on dunes on marine terraces, coastal plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67292:1113168"|"67292:961593"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Yaquina component makes up 85 percent of the map unit. Slopes are 0 to 5 percent. This component is on coastal plains, depressions. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil meets hydric criteria."|"67293:1113169"|"67293:961641"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Heceta soil is a minor component."|"67293:1151313"|"67293:1687060"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Humaquepts soil is a minor component."|"67293:1151315"|"67293:1687061"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Heceta component makes up 85 percent of the map unit. Slopes are 0 to 3 percent. This component is on depressions on interdunes, coastal plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, November, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4w.  This soil meets hydric criteria."|"67294:1113173"|"67294:798097"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Humaquepts soil is a minor component."|"67294:1137602"|"67294:1687065"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Lebam component makes up 85 percent of the map unit. Slopes are 3 to 12 percent. This component is on mountains, hillslopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67295:1768219"|"67295:2208115"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Sevencedars, till substratum component makes up 85 percent of the map unit. Slopes are 60 to 90 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium overlying glacial till derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"67296:129022"|"67296:88931"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Alic Hapludands, fan component makes up 35 percent of the map unit. Slopes are 3 to 15 percent. This component is on fans, valleys. The parent material consists of debris flow deposits derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67297:1106042"|"67297:1687257"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Alic Hapludands, terrace component makes up 60 percent of the map unit. Slopes are 3 to 15 percent. This component is on stream terraces, valleys. The parent material consists of alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 37 to 61 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria."|"67297:1130306"|"67297:1687256"
08/12/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Croquib soil is a minor component."|"67297:1130510"|"67297:1687258"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Svensen component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67300:1161424"|"67300:1687396"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Walluski component makes up 85 percent of the map unit. Slopes are 7 to 15 percent. This component is on stream terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 27 inches during January, February, March, April, November, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"67301:1161428"|"67301:1687399"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"67301:1585279"|"67301:1687400"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldport component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on dunes on coastal plains, dunes on marine terraces. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67302:1178737"|"67302:1687047"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Heceta soil is a minor component."|"67302:1318651"|"67302:1687048"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Udorthents, flooded component makes up 25 percent of the map unit. Slopes are 0 to 7 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock and/or colluvium derived from igneous rock and human transported materials. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 14 inches during January, February, March, April, May, November, December. Organic matter content in the surface horizon is about 6 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"67304:1113278"|"67304:1687231"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Urban land is a miscellaneous area."|"67304:1113279"|"67304:1687230"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Aquepts soil is a minor component."|"67304:1345242"|"67304:1687232"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Coquille, protected component makes up 50 percent of the map unit. Slopes are 0 to 1 percent. This component is on estuaries, lowlands. The parent material consists of estuarine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is rarely flooded. It is frequently ponded. A seasonal zone of water saturation is at 14 inches during January, February, December. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria."|"67305:1113285"|"67305:965960"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Nehalem, protected component makes up 15 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, lowlands. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 2w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria."|"67305:1152071"|"67305:1687242"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Brenner, protected component makes up 30 percent of the map unit. Slopes are 0 to 1 percent. This component is on lowlands, flood plains. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is frequently ponded. A seasonal zone of water saturation is at 14 inches during January, February, March, April, May, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil meets hydric criteria."|"67305:1544223"|"67305:1687241"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Udifluvents component makes up 40 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 4w.  This soil does not meet hydric criteria."|"67306:1113274"|"67306:1687203"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Fluvaquents soil is a minor component."|"67306:1147976"|"67306:1687206"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"67306:1147977"|"67306:1687204"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"67306:1147978"|"67306:1687205"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Yachats component makes up 85 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria."|"67307:1113275"|"67307:1687207"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"67307:1152044"|"67307:1687208"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Necanicum component makes up 25 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock and tuff. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67309:1113207"|"67309:1687097"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 60 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"67309:1113208"|"67309:1687096"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldport, thin surface component makes up 85 percent of the map unit. Slopes are 60 to 90 percent. This component is on dunes on coastal plains, dunes on marine terraces. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"741651:1105057"|"741651:1687243"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Hebo component makes up 80 percent of the map unit. Slopes are 0 to 5 percent. This component is on depressions on stream terraces, drainageways on fluviomarine terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, December. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 4e.  This soil meets hydric criteria."|"741676:1106716"|"741676:963252"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Aquepts soil is a minor component."|"741676:1151679"|"741676:1687133"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Croquib soil is a minor component."|"741676:1342550"|"741676:1687134"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Condorbridge component makes up 80 percent of the map unit. Slopes are 3 to 15 percent. This component is on fans, river valleys. The parent material consists of alluvium and/or debris flow deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 20 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"741677:1139106"|"741677:1687158"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Wolfer component makes up 85 percent of the map unit. Slopes are 3 to 15 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium overlying sandy and gravelly alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 24 to 36 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 3s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"741678:1112326"|"741678:963537"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"741678:1151704"|"741678:1687155"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Quillamook, gravelly substratum component makes up 60 percent of the map unit. Slopes are 3 to 15 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium overlying sandy and gravelly alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 17 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"741679:1198229"|"741679:1687200"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Quillamook component makes up 25 percent of the map unit. Slopes are 3 to 15 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 17 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"741679:1198230"|"741679:1687201"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"741679:1343523"|"741679:1687202"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Gauldy component makes up 85 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 30 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria."|"741680:1150878"|"741680:1687209"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"741680:1152049"|"741680:1687210"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"741681:1152060"|"741681:1687213"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Gauldy component makes up 40 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 30 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria."|"741681:1152061"|"741681:1687212"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Yachats component makes up 45 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria."|"741681:1152062"|"741681:1687211"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Munsoncreek component makes up 30 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"741686:1150887"|"741686:1687260"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fendall component makes up 50 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 12 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"741686:1150889"|"741686:1687259"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Aquepts soil is a minor component."|"741686:1293382"|"741686:1687261"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Aquepts component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 5w.  This soil meets hydric criteria."|"741688:1106825"|"741688:805293"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Dystrudepts component makes up 25 percent of the map unit. Slopes are 0 to 5 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 63 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 2e.  This soil does not meet hydric criteria."|"741688:1106826"|"741688:804987"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fluventic Humic Dystrudepts component makes up 45 percent of the map unit. Slopes are 0 to 5 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 61 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 35 inches during January, February, March, April, May, November, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"741688:1106827"|"741688:804982"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Humaquepts soil is a minor component."|"741688:1348848"|"741688:1687335"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Salander component makes up 25 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes, hillslopes. The parent material consists of colluvium and resdiuum derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"741689:1150895"|"741689:1687343"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Neskowin component makes up 60 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes, hillslopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"741689:1150896"|"741689:1687342"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fendall component makes up 30 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 12 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"741690:1152604"|"741690:1687350"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Winema component makes up 55 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 12 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"741690:1152605"|"741690:1687349"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Salander component makes up 30 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and resdiuum derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"741691:1152597"|"741691:1687348"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Neotsu component makes up 60 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and residuum derived from igneous rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"741691:1152598"|"741691:1687347"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Siletz component makes up 80 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"741692:1106011"|"741692:960967"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"741692:1152243"|"741692:1687263"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Templeton component makes up 55 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"747146:1106568"|"747146:946660"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Skipanon component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of mass movement deposits derived from a mixture of igneous and sedimentary rock types overlying sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"747146:1106573"|"747146:1687120"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Chitwood component makes up 30 percent of the map unit. Slopes are 3 to 15 percent. This component is on stream terraces, fluviomarine terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 11 inches during January, February, December. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"801115:1150917"|"801115:1687146"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Walluski component makes up 45 percent of the map unit. Slopes are 3 to 15 percent. This component is on stream terraces, fluviomarine terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 27 inches during January, February, March, April, November, December. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"801115:1150918"|"801115:1687145"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"801115:1150919"|"801115:1687147"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"801121:1150931"|"801121:1687352"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Udorthents, steep component makes up 50 percent of the map unit. Slopes are 60 to 100 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria."|"801121:1150932"|"801121:1687351"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Dystrudepts, steep component makes up 95 percent of the map unit. Slopes are 25 to 60 percent. This component is on escarpments on stream terraces, river valleys. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"801123:1152608"|"801123:1687372"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Winema component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 12 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"801127:1161458"|"801127:1687415"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Fendall component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, hillslopes. The parent material consists of colluvium and residuum derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 12 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria."|"801127:1161459"|"801127:1687414"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Chitwood component makes up 80 percent of the map unit. Slopes are 7 to 15 percent. This component is on stream terraces, fluviomarine terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 11 inches during January, February, December. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"996247:1198188"|"996247:1687075"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"996247:1341526"|"996247:1687076"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolovana component makes up 85 percent of the map unit. Slopes are 5 to 30 percent. This component is on mountains, hillslopes, mountain slopes. The parent material consists of colluvium and residuum derived from tuffaceous sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"996294:1198192"|"996294:1687116"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Knappa component makes up 85 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, fluviomarine terraces, river valleys. The parent material consists of mixed alluvium and/or fluviomarine deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 9 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"996295:1198207"|"996295:1687148"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"996295:1342772"|"996295:1687149"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Wolfer component makes up 80 percent of the map unit. Slopes are 0 to 5 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium overlying sandy and gravelly alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 24 to 36 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 3s. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"996296:1198210"|"996296:1687152"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"996296:1245462"|"996296:1687153"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Condorbridge component makes up 85 percent of the map unit. Slopes are 0 to 7 percent. This component is on fans, river valleys. The parent material consists of alluvium and/or debris flow deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 20 percent.  Nonirrigated land capability classification is 2e.  This soil does not meet hydric criteria."|"996297:1198219"|"996297:1687156"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"996297:1340609"|"996297:1687157"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Urban land is a miscellaneous area."|"997489:1198325"|"997489:1687219"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Quillamook component makes up 30 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 17 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"997489:1198327"|"997489:1687218"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"997489:1344983"|"997489:1687220"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ginger component makes up 35 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 17 inches during January, February, December. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"997489:1543478"|"997489:1687217"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Quillamook component makes up 30 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 17 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"997491:1198328"|"997491:1687222"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Urban land is a miscellaneous area."|"997491:1198329"|"997491:1687221"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"997491:1345125"|"997491:1687223"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Siletz, warm component makes up 80 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"997494:1198333"|"997494:1687264"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"997494:1340823"|"997494:1687265"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Wolfer component makes up 40 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of silty alluvium overlying sandy and gravelly alluvium derived from igneous rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 24 to 36 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 3s. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"997495:1198335"|"997495:1687268"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Siletz component makes up 45 percent of the map unit. Slopes are 0 to 7 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"997495:1198336"|"997495:1687267"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"997495:1347437"|"997495:1687269"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Condorbridge, warm component makes up 80 percent of the map unit. Slopes are 3 to 15 percent. This component is on fans, valleys. The parent material consists of alluvium and/or debris flow deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 20 percent.  Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria."|"997496:1198334"|"997496:1687266"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Nehalem, occasional component makes up 40 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 8 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"997498:1198367"|"997498:1687313"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Logsden component makes up 50 percent of the map unit. Slopes are 0 to 5 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 7 percent.  Nonirrigated land capability classification is 2e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria."|"997498:1198368"|"997498:1687312"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brenner soil is a minor component."|"997498:1323534"|"997498:1687314"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hebo soil is a minor component."|"997499:1348544"|"997499:1687320"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Tillamook component makes up 45 percent of the map unit. Slopes are 3 to 15 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 25 inches during January, February, March, December. Organic matter content in the surface horizon is about 17 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"997499:1543112"|"997499:1687318"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Ginger component makes up 40 percent of the map unit. Slopes are 3 to 15 percent. This component is on stream terraces, river valleys. The parent material consists of alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 17 inches during January, February, December. Organic matter content in the surface horizon is about 15 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria."|"997499:1543476"|"997499:1687319"
08/11/2009|"Nontechnical description"|"GENSOIL"|"generated"|"The Mulkey component makes up 85 percent of the map unit. Slopes are 3 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of loamy colluvium and residuum derived from basalt or other coarse-grained intrusive igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 14 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria."|"997500:129177"|"997500:752572"
